complexType RecordingEventDefinitionsType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | Enabled ChannelID InternalEventsEnabled RecordingEvent RecordingIndex RecorderControl
used by |
element | RecorderReproducerAttributesType/RecordingEventDefinitions
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="RecordingEventDefinitionsType"> <xs:sequence minOccurs="0"> <xs:element name="Enabled" type="TmatsCommon:TrueFalseType" default="False" minOccurs="0"> <xs:annotation> <xs:documentation>EV\E</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ChannelID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\TK1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InternalEventsEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\IEE</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecordingEvent" type="RecordingEventType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats EV\N times</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecordingIndex" type="RecordingIndexType" minOccurs="0"/> <xs:element name="RecorderControl" type="RecorderControlType" minOccurs="0"/> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element RecordingEventDefinitionsType/Enabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | False
facets |
enumeration | True
enumeration | False
annotation |
documentation
EV\E
source | <xs:element name="Enabled" type="TmatsCommon:TrueFalseType" default="False" minOccurs="0"> <xs:annotation> <xs:documentation>EV\E</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventDefinitionsType/ChannelID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\TK1
source | <xs:element name="ChannelID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\TK1</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventDefinitionsType/InternalEventsEnabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
EV\IEE
source | <xs:element name="InternalEventsEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\IEE</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventDefinitionsType/RecordingEvent

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | RecordingEventType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | ID Description DataProcessingEnabled Type Priority EventCaptureMode EventInitialCapture LimitCount TriggerMeasurement EventProcessing
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeats EV\N times
source | <xs:element name="RecordingEvent" type="RecordingEventType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats EV\N times</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventDefinitionsType/RecordingIndex

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | RecordingIndexType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Enabled ChannelID Type TimeValue CountValue
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="RecordingIndex" type="RecordingIndexType" minOccurs="0"/>

element RecordingEventDefinitionsType/RecorderControl

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | RecorderControlType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | MessageMonitorRecordControlEnabled ChannelID MessageRecordControlType StopPauseCommandWord StartResumeCommandWord
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="RecorderControl" type="RecorderControlType" minOccurs="0"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy