complexType UARTSubChannelType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | Number Name BaudRate BitsPerWord Parity StopBits Interface BlockSize SyncWordLength BlockSyncValue BlockRate
used by |
element | UARTDataTypeAttributesType/SubChannel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="UARTSubChannelType"> <xs:sequence minOccurs="0"> <xs:element name="Number" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>USCN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>UCNM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BaudRate" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>UCR</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BitsPerWord" minOccurs="0"> <xs:annotation> <xs:documentation>UCB</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:integer"> <xs:minInclusive value="7"/> <xs:maxInclusive value="9"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="Parity" type="TmatsCommon:OddEvenNoneType" minOccurs="0"> <xs:annotation> <xs:documentation>UCP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="StopBits" type="TmatsCommon:UARTStopBitsType" minOccurs="0"> <xs:annotation> <xs:documentation>UCS</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Interface" type="TmatsCommon:UARTInterfaceType" minOccurs="0"> <xs:annotation> <xs:documentation>UCIN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BlockSize" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>UCBS</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SyncWordLength" minOccurs="0"> <xs:annotation> <xs:documentation>UCSL</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="9"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="BlockSyncValue" type="TmatsCommon:BinaryType" minOccurs="0"> <xs:annotation> <xs:documentation>UCSV</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BlockRate" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>UCBR</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element UARTSubChannelType/Number

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
USCN
source | <xs:element name="Number" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>USCN</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/Name

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
UCNM
source | <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>UCNM</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/BaudRate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:double
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
UCR
source | <xs:element name="BaudRate" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>UCR</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/BitsPerWord

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | restriction of xs:integer
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
minInclusive | 7
maxInclusive | 9
annotation |
documentation
UCB
source | <xs:element name="BitsPerWord" minOccurs="0"> <xs:annotation> <xs:documentation>UCB</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:integer"> <xs:minInclusive value="7"/> <xs:maxInclusive value="9"/> </xs:restriction> </xs:simpleType> </xs:element>

element UARTSubChannelType/Parity

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:OddEvenNoneType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
UCP
source | <xs:element name="Parity" type="TmatsCommon:OddEvenNoneType" minOccurs="0"> <xs:annotation> <xs:documentation>UCP</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/StopBits

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:UARTStopBitsType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | 1.0
enumeration | 1.5
enumeration | 2.0
annotation |
documentation
UCS
source | <xs:element name="StopBits" type="TmatsCommon:UARTStopBitsType" minOccurs="0"> <xs:annotation> <xs:documentation>UCS</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/Interface

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:UARTInterfaceType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Other
enumeration | RS-232
enumeration | RS-422
enumeration | RS-485
enumeration | TTL
annotation |
documentation
UCIN
source | <xs:element name="Interface" type="TmatsCommon:UARTInterfaceType" minOccurs="0"> <xs:annotation> <xs:documentation>UCIN</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/BlockSize

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
UCBS
source | <xs:element name="BlockSize" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>UCBS</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/SyncWordLength

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | restriction of xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
minInclusive | 0
maxInclusive | 9
annotation |
documentation
UCSL
source | <xs:element name="SyncWordLength" minOccurs="0"> <xs:annotation> <xs:documentation>UCSL</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="9"/> </xs:restriction> </xs:simpleType> </xs:element>

element UARTSubChannelType/BlockSyncValue

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:BinaryType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-1]*
annotation |
documentation
UCSV
source | <xs:element name="BlockSyncValue" type="TmatsCommon:BinaryType" minOccurs="0"> <xs:annotation> <xs:documentation>UCSV</xs:documentation> </xs:annotation> </xs:element>

element UARTSubChannelType/BlockRate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:double
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
UCBR
source | <xs:element name="BlockRate" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>UCBR</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy