complexType CompositeSignalStructureType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
children | TmatsM:SignalStructureType TmatsM:ModulationSense TmatsM:CompositeLPFBandwidth
used by |
element | MultiplexModulationGroupType/CompositeSignalStructure
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="CompositeSignalStructureType"> <xs:sequence minOccurs="0"> <xs:element name="SignalStructureType" type="TmatsCommon:SignalStructureTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>BB1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ModulationSense" type="TmatsCommon:PositiveNegative" minOccurs="0"> <xs:annotation> <xs:documentation>BB2</xs:documentation> </xs:annotation> </xs:element> <xs:element name="CompositeLPFBandwidth" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>BB3</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element CompositeSignalStructureType/SignalStructureType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | TmatsCommon:SignalStructureTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | PCM
enumeration | Analog
enumeration | SCO's
enumeration | ANA/SCO
enumeration | PCM/SCO
enumeration | Other
annotation |
documentation
BB1
source | <xs:element name="SignalStructureType" type="TmatsCommon:SignalStructureTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>BB1</xs:documentation> </xs:annotation> </xs:element>

element CompositeSignalStructureType/ModulationSense

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | TmatsCommon:PositiveNegative
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Positive
enumeration | Negative
annotation |
documentation
BB2
source | <xs:element name="ModulationSense" type="TmatsCommon:PositiveNegative" minOccurs="0"> <xs:annotation> <xs:documentation>BB2</xs:documentation> </xs:annotation> </xs:element>

element CompositeSignalStructureType/CompositeLPFBandwidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
BB3
source | <xs:element name="CompositeLPFBandwidth" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>BB3</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy