complexType PCMDataTypeAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | DataTypeFormat DataPackingOption InputClockEdge InputSignalType InputThreshold InputTermination VideoTypeFormat MinorFrameFilteringEnabled PostProcessOverwriteAndFiltering MinorFrameFiltering MeasurementOverwrite
used by |
element | DataType/PCMDataTypeAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="PCMDataTypeAttributesType"> <xs:sequence minOccurs="0"> <xs:element name="DataTypeFormat" type="TmatsCommon:PCMDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>PDTF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataPackingOption" type="TmatsCommon:PCMDataPackingOptionType" minOccurs="0"> <xs:annotation> <xs:documentation>PDP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputClockEdge" type="TmatsCommon:PCMDataClockEdgeType" default="0 Degrees" minOccurs="0"> <xs:annotation> <xs:documentation>ICE</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputSignalType" type="TmatsCommon:PCMDataInputSignalTypeType" default="Differential" minOccurs="0"> <xs:annotation> <xs:documentation>IST</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputThreshold" type="xs:float" minOccurs="0"> <xs:annotation> <xs:documentation>ITH</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputTermination" type="TmatsCommon:InputTerminationType" minOccurs="0"> <xs:annotation> <xs:documentation>ITM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="VideoTypeFormat" type="TmatsCommon:VideoTypeFormatType" default="None" minOccurs="0"> <xs:annotation> <xs:documentation>PTF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MinorFrameFilteringEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>MFF\E</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PostProcessOverwriteAndFiltering" type="PostProcessOverwriteAndFilteringType" minOccurs="0"/> <xs:element name="MinorFrameFiltering" type="MinorFrameFilteringType" minOccurs="0"/> <xs:element name="MeasurementOverwrite" type="MeasurementOverwriteType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>SMF\SMN and SMF\MFOT. Repeats SMF\N-n times</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element PCMDataTypeAttributesType/DataTypeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:PCMDataTypeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Format 0 (Reserved)
enumeration | Format 1 (IRIG 106 Ch 4/8)
annotation |
documentation
PDTF
source | <xs:element name="DataTypeFormat" type="TmatsCommon:PCMDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>PDTF</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/DataPackingOption

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:PCMDataPackingOptionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Unpacked
enumeration | Packed With Frame Sync
enumeration | Throughput Mode
annotation |
documentation
PDP
source | <xs:element name="DataPackingOption" type="TmatsCommon:PCMDataPackingOptionType" minOccurs="0"> <xs:annotation> <xs:documentation>PDP</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/InputClockEdge

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:PCMDataClockEdgeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 0 Degrees
facets |
enumeration | 0 Degrees
enumeration | 180 Degrees
annotation |
documentation
ICE
source | <xs:element name="InputClockEdge" type="TmatsCommon:PCMDataClockEdgeType" default="0 Degrees" minOccurs="0"> <xs:annotation> <xs:documentation>ICE</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/InputSignalType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:PCMDataInputSignalTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Differential
facets |
enumeration | Single Ended
enumeration | Differential
enumeration | RS-422 Standard Differential
enumeration | Single Ended With TTL
annotation |
documentation
IST
source | <xs:element name="InputSignalType" type="TmatsCommon:PCMDataInputSignalTypeType" default="Differential" minOccurs="0"> <xs:annotation> <xs:documentation>IST</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/InputThreshold

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:float
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ITH
source | <xs:element name="InputThreshold" type="xs:float" minOccurs="0"> <xs:annotation> <xs:documentation>ITH</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/InputTermination

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:InputTerminationType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Low-Z
enumeration | High-Z
annotation |
documentation
ITM
source | <xs:element name="InputTermination" type="TmatsCommon:InputTerminationType" minOccurs="0"> <xs:annotation> <xs:documentation>ITM</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/VideoTypeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:VideoTypeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | None
facets |
enumeration | None
enumeration | MPEG1
enumeration | MPEG2
enumeration | H261
enumeration | WAVE
enumeration | Other
annotation |
documentation
PTF
source | <xs:element name="VideoTypeFormat" type="TmatsCommon:VideoTypeFormatType" default="None" minOccurs="0"> <xs:annotation> <xs:documentation>PTF</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/MinorFrameFilteringEnabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
MFF\E
source | <xs:element name="MinorFrameFilteringEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>MFF\E</xs:documentation> </xs:annotation> </xs:element>

element PCMDataTypeAttributesType/PostProcessOverwriteAndFiltering

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | PostProcessOverwriteAndFilteringType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Enabled Type
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="PostProcessOverwriteAndFiltering" type="PostProcessOverwriteAndFilteringType" minOccurs="0"/>

element PCMDataTypeAttributesType/MinorFrameFiltering

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | MinorFrameFilteringType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Type MinorFrameNumber
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="MinorFrameFiltering" type="MinorFrameFilteringType" minOccurs="0"/>

element PCMDataTypeAttributesType/MeasurementOverwrite

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | MeasurementOverwriteType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Measurement OverwriteTag
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
SMF\SMN and SMF\MFOT. Repeats SMF\N-n times
source | <xs:element name="MeasurementOverwrite" type="MeasurementOverwriteType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>SMF\SMN and SMF\MFOT. Repeats SMF\N-n times</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy