complexType DataType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | TrackNumberOrChannelID RecordingTechnique InputStreamDerandomized DataSourceID DataDirection RecorderPhysicalChannelNumber ChannelEnable ChannelDataType ChannelDataLinkName SecondaryHeaderTimeFormat PCMDataTypeAttributes MIL-STD-1553BusDataTypeAttributes AnalogDataTypeAttributes DiscreteDataTypeAttributes ARINC429BusDataTypeAttributes VideoDataTypeAttributes TimeDataTypeAttributes ImageDataTypeAttributes UARTDataTypeAttributes MessageDataTypeAttributes IEEE1394DataTypeAttributes ParallelDataTypeAttributes EthernetDataTypeAttributes TSPICTSDataTypeAttributes CanBusDataTypeAttributes FibreChannelDataTypeAttributes TelemetryOutputAttributes
used by |
element | RecorderReproducerAttributesType/Data
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="DataType"> <xs:sequence minOccurs="0"> <xs:element name="TrackNumberOrChannelID" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>TK1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecordingTechnique" type="TmatsCommon:RecordingTechniqueType" minOccurs="0"> <xs:annotation> <xs:documentation>TK2</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputStreamDerandomized" type="TmatsCommon:YesNoType" default="No" minOccurs="0"> <xs:annotation> <xs:documentation>IDDR</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataSourceID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>DSI</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataDirection" type="TmatsCommon:DataDirectionType" default="Forward" minOccurs="0"> <xs:annotation> <xs:documentation>TK3</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecorderPhysicalChannelNumber" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>TK4</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ChannelEnable" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>CHE</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ChannelDataType" type="TmatsCommon:ChannelDataTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>CDT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ChannelDataLinkName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>CDLN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SecondaryHeaderTimeFormat" type="TmatsCommon:SecondaryHeaderTimeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>SHTF</xs:documentation> </xs:annotation> </xs:element> <xs:choice minOccurs="0"> <xs:annotation> <xs:documentation>Based upon value of ChannelDataType</xs:documentation> </xs:annotation> <xs:element name="PCMDataTypeAttributes" type="PCMDataTypeAttributesType" minOccurs="0"/> <xs:element name="MIL-STD-1553BusDataTypeAttributes" type="MIL-STD-1553BusDataTypeAttributesType" minOccurs="0"/> <xs:element name="AnalogDataTypeAttributes" type="AnalogDataTypeAttributesType" minOccurs="0"/> <xs:element name="DiscreteDataTypeAttributes" type="DiscreteDataTypeAttributesType" minOccurs="0"/> <xs:element name="ARINC429BusDataTypeAttributes" type="ARINC429BusDataTypeAttributesType" minOccurs="0"/> <xs:element name="VideoDataTypeAttributes" type="VideoDataTypeAttributesType" minOccurs="0"/> <xs:element name="TimeDataTypeAttributes" type="TimeDataTypeAttributesType" minOccurs="0"/> <xs:element name="ImageDataTypeAttributes" type="ImageDataTypeAttributesType" minOccurs="0"/> <xs:element name="UARTDataTypeAttributes" type="UARTDataTypeAttributesType" minOccurs="0"/> <xs:element name="MessageDataTypeAttributes" type="MessageDataTypeAttributesType" minOccurs="0"/> <xs:element name="IEEE1394DataTypeAttributes" type="IEEE1394DataTypeAttributesType" minOccurs="0"/> <xs:element name="ParallelDataTypeAttributes" type="ParallelDataTypeAttributesType" minOccurs="0"/> <xs:element name="EthernetDataTypeAttributes" type="EthernetDataTypeAttributesType" minOccurs="0"/> <xs:element name="TSPICTSDataTypeAttributes" type="TSPICTSDataTypeAttributesType" minOccurs="0"/> <xs:element name="CanBusDataTypeAttributes" type="CanBusDataTypeAttributesType" minOccurs="0"/> <xs:element name="FibreChannelDataTypeAttributes" type="FibreChannelDataTypeAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TelemetryOutputAttributes" type="TelemetryOutputAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element> </xs:choice> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element DataType/TrackNumberOrChannelID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
TK1
source | <xs:element name="TrackNumberOrChannelID" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>TK1</xs:documentation> </xs:annotation> </xs:element>

element DataType/RecordingTechnique

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:RecordingTechniqueType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | FM/FM
enumeration | HDDR
enumeration | Pre-Detection
enumeration | Direct
enumeration | FM Wide Band Group 1
enumeration | FM Wide band Group 2
enumeration | FM Intermediate Band
enumeration | FM Narrow Band
enumeration | Double Density
enumeration | Rotary Single Track
enumeration | Rotary Multiplexed
enumeration | Solid State
enumeration | Other
annotation |
documentation
TK2
source | <xs:element name="RecordingTechnique" type="TmatsCommon:RecordingTechniqueType" minOccurs="0"> <xs:annotation> <xs:documentation>TK2</xs:documentation> </xs:annotation> </xs:element>

element DataType/InputStreamDerandomized

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:YesNoType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | No
facets |
enumeration | Yes
enumeration | No
annotation |
documentation
IDDR
source | <xs:element name="InputStreamDerandomized" type="TmatsCommon:YesNoType" default="No" minOccurs="0"> <xs:annotation> <xs:documentation>IDDR</xs:documentation> </xs:annotation> </xs:element>

element DataType/DataSourceID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
DSI
source | <xs:element name="DataSourceID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>DSI</xs:documentation> </xs:annotation> </xs:element>

element DataType/DataDirection

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:DataDirectionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Forward
facets |
enumeration | Forward
enumeration | Reverse
annotation |
documentation
TK3
source | <xs:element name="DataDirection" type="TmatsCommon:DataDirectionType" default="Forward" minOccurs="0"> <xs:annotation> <xs:documentation>TK3</xs:documentation> </xs:annotation> </xs:element>

element DataType/RecorderPhysicalChannelNumber

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
TK4
source | <xs:element name="RecorderPhysicalChannelNumber" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>TK4</xs:documentation> </xs:annotation> </xs:element>

element DataType/ChannelEnable

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
CHE
source | <xs:element name="ChannelEnable" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>CHE</xs:documentation> </xs:annotation> </xs:element>

element DataType/ChannelDataType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:ChannelDataTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | PCM Input
enumeration | Analog Input
enumeration | Discrete Input
enumeration | Time Input
enumeration | Video Input
enumeration | UART Input
enumeration | 1553 Input
enumeration | ARINC-429 Input
enumeration | Message Data Input
enumeration | Image Data Input
enumeration | IEEE 1394 Input
enumeration | Parallel Input
enumeration | Ethernet Input
enumeration | TSPI/CTS Input
enumeration | Can Bus Input
enumeration | Fibre Channel Input
enumeration | Telemetry Output
annotation |
documentation
CDT
source | <xs:element name="ChannelDataType" type="TmatsCommon:ChannelDataTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>CDT</xs:documentation> </xs:annotation> </xs:element>

element DataType/ChannelDataLinkName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
CDLN
source | <xs:element name="ChannelDataLinkName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>CDLN</xs:documentation> </xs:annotation> </xs:element>

element DataType/SecondaryHeaderTimeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:SecondaryHeaderTimeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | IRIG-106 Chapter 4 BCD
enumeration | IEEE-1588
enumeration | ERTC
annotation |
documentation
SHTF
source | <xs:element name="SecondaryHeaderTimeFormat" type="TmatsCommon:SecondaryHeaderTimeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>SHTF</xs:documentation> </xs:annotation> </xs:element>

element DataType/PCMDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | PCMDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat DataPackingOption InputClockEdge InputSignalType InputThreshold InputTermination VideoTypeFormat MinorFrameFilteringEnabled PostProcessOverwriteAndFiltering MinorFrameFiltering MeasurementOverwrite
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="PCMDataTypeAttributes" type="PCMDataTypeAttributesType" minOccurs="0"/>

element DataType/MIL-STD-1553BusDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | MIL-STD-1553BusDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | BusDataTypeFormat FilteringEnabled PostProcessOverwriteAndFilteringEnabled MessageFilteringType MessageFilteringDefinitions MeasurementOverwriteDefinitions
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="MIL-STD-1553BusDataTypeAttributes" type="MIL-STD-1553BusDataTypeAttributesType" minOccurs="0"/>

element DataType/AnalogDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | AnalogDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat DataPackingOption SampleRate Channel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="AnalogDataTypeAttributes" type="AnalogDataTypeAttributesType" minOccurs="0"/>

element DataType/DiscreteDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | DiscreteDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat DiscreteMode SampleRate Measurement
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="DiscreteDataTypeAttributes" type="DiscreteDataTypeAttributesType" minOccurs="0"/>

element DataType/ARINC429BusDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | ARINC429BusDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat SubChannel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="ARINC429BusDataTypeAttributes" type="ARINC429BusDataTypeAttributesType" minOccurs="0"/>

element DataType/VideoDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | VideoDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat MPEG2ChannelXON2Format SignalType SignalFormatType ConstantBitRate VariablePeakBitRate EncodingDelay Overlay AudioChannelInput VideoDataAlignment
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="VideoDataTypeAttributes" type="VideoDataTypeAttributesType" minOccurs="0"/>

element DataType/TimeDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TimeDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat TimeFormat TimeSource
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="TimeDataTypeAttributes" type="TimeDataTypeAttributesType" minOccurs="0"/>

element DataType/ImageDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | ImageDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat StillImageType DynamicImageFormat TimeStampMode DynamicImageAcquisitionMode ImageFrameRate PreTriggerFrames TotalFrames ExposureTime SensorRotation SensorGain SensorAutoGain SensorWidth SensorHeight MaximumImageWidth MaximumImageHeight ImageWidth ImageHeight ImageOffsetX ImageOffsetY LinePitch BinningHorizontal BinningVertical DecimationHorizontal DecimationVertical ReverseX ReverseY PixelDynamicRangeMinimum PixelDynamicRangeMaximum TestImageType
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="ImageDataTypeAttributes" type="ImageDataTypeAttributesType" minOccurs="0"/>

element DataType/UARTDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | UARTDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat SubChannel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="UARTDataTypeAttributes" type="UARTDataTypeAttributesType" minOccurs="0"/>

element DataType/MessageDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | MessageDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat SubChannel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="MessageDataTypeAttributes" type="MessageDataTypeAttributesType" minOccurs="0"/>

element DataType/IEEE1394DataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | IEEE1394DataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="IEEE1394DataTypeAttributes" type="IEEE1394DataTypeAttributesType" minOccurs="0"/>

element DataType/ParallelDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | ParallelDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="ParallelDataTypeAttributes" type="ParallelDataTypeAttributesType" minOccurs="0"/>

element DataType/EthernetDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | EthernetDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat Network
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="EthernetDataTypeAttributes" type="EthernetDataTypeAttributesType" minOccurs="0"/>

element DataType/TSPICTSDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TSPICTSDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Format
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="TSPICTSDataTypeAttributes" type="TSPICTSDataTypeAttributesType" minOccurs="0"/>

element DataType/CanBusDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | CanBusDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataTypeFormat SubChannel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="CanBusDataTypeAttributes" type="CanBusDataTypeAttributesType" minOccurs="0"/>

element DataType/FibreChannelDataTypeAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | FibreChannelDataTypeAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | FibreChannelDataTypeFormat FibreChannelSpeed
annotation |
documentation
Added in 106-15
source | <xs:element name="FibreChannelDataTypeAttributes" type="FibreChannelDataTypeAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

element DataType/TelemetryOutputAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TelemetryOutputAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | OutputStreamName StreamID ConfigurationPacketHashCodeRate ConfigurationPacketRate
annotation |
documentation
Added in 106-15
source | <xs:element name="TelemetryOutputAttributes" type="TelemetryOutputAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy