complexType ChannelType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | SubChannelEnabled SubChannelNumber MeasurementName DataLength BitMask MeasurementTransferOrder SampleFactor SampleFilter3dbBandwidth Coupling RecorderInputImpedance InputChannelGain InputFullScaleRange InputOffsetVoltage RecordedAnalogFormat InputType Audio AudioFormat
used by |
element | AnalogDataTypeAttributesType/Channel
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="ChannelType"> <xs:sequence minOccurs="0"> <xs:element name="SubChannelEnabled" type="TmatsCommon:TrueFalseType" default="True" minOccurs="0"> <xs:annotation> <xs:documentation>AMCE - Added in 106-15</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SubChannelNumber"> <xs:annotation> <xs:documentation>AMCN - Added in 106-15</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:int"> <xs:minInclusive value="1"/> <xs:maxInclusive value="256"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="MeasurementName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>AMN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataLength" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADL</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BitMask" type="TmatsCommon:MeasurementBitMaskType" default="Full Word" minOccurs="0"> <xs:annotation> <xs:documentation>AMSK</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MeasurementTransferOrder" type="TmatsCommon:MSBLSBFirstType" default="MSB First" minOccurs="0"> <xs:annotation> <xs:documentation>AMTO</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SampleFactor" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ASF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SampleFilter3dbBandwidth" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ASBW</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Coupling" type="TmatsCommon:AnalogCouplingType" minOccurs="0"> <xs:annotation> <xs:documentation>ACP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecorderInputImpedance" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AII</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputChannelGain" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AGI</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputFullScaleRange" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AFSI</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputOffsetVoltage" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AOVI</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecordedAnalogFormat" type="TmatsCommon:AnalogRecordedFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>AF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="InputType" type="TmatsCommon:AnalogInputTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>AIT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Audio" type="TmatsCommon:AnalogAudioType" minOccurs="0"> <xs:annotation> <xs:documentation>AV</xs:documentation> </xs:annotation> </xs:element> <xs:element name="AudioFormat" type="TmatsCommon:AnalogAudioFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>AVF</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element ChannelType/SubChannelEnabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | True
facets |
enumeration | True
enumeration | False
annotation |
documentation
AMCE - Added in 106-15
source | <xs:element name="SubChannelEnabled" type="TmatsCommon:TrueFalseType" default="True" minOccurs="0"> <xs:annotation> <xs:documentation>AMCE - Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/SubChannelNumber

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | restriction of xs:int
properties |
isRef | 0
content | simple
facets |
minInclusive | 1
maxInclusive | 256
annotation |
documentation
AMCN - Added in 106-15
source | <xs:element name="SubChannelNumber"> <xs:annotation> <xs:documentation>AMCN - Added in 106-15</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:int"> <xs:minInclusive value="1"/> <xs:maxInclusive value="256"/> </xs:restriction> </xs:simpleType> </xs:element>

element ChannelType/MeasurementName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AMN
source | <xs:element name="MeasurementName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>AMN</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/DataLength

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ADL
source | <xs:element name="DataLength" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADL</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/BitMask

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:MeasurementBitMaskType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Full Word
facets |
pattern | [0-1]*
pattern | Full Word
annotation |
documentation
AMSK
source | <xs:element name="BitMask" type="TmatsCommon:MeasurementBitMaskType" default="Full Word" minOccurs="0"> <xs:annotation> <xs:documentation>AMSK</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/MeasurementTransferOrder

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:MSBLSBFirstType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | MSB First
facets |
enumeration | MSB First
enumeration | LSB First
annotation |
documentation
AMTO
source | <xs:element name="MeasurementTransferOrder" type="TmatsCommon:MSBLSBFirstType" default="MSB First" minOccurs="0"> <xs:annotation> <xs:documentation>AMTO</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/SampleFactor

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ASF
source | <xs:element name="SampleFactor" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ASF</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/SampleFilter3dbBandwidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ASBW
source | <xs:element name="SampleFilter3dbBandwidth" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ASBW</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/Coupling

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogCouplingType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | AC
enumeration | DC
annotation |
documentation
ACP
source | <xs:element name="Coupling" type="TmatsCommon:AnalogCouplingType" minOccurs="0"> <xs:annotation> <xs:documentation>ACP</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/RecorderInputImpedance

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AII
source | <xs:element name="RecorderInputImpedance" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AII</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/InputChannelGain

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AGI
source | <xs:element name="InputChannelGain" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AGI</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/InputFullScaleRange

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AFSI
source | <xs:element name="InputFullScaleRange" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AFSI</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/InputOffsetVoltage

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AOVI
source | <xs:element name="InputOffsetVoltage" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AOVI</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/RecordedAnalogFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogRecordedFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | One's Complement
enumeration | Two's Complement
enumeration | Sign and Magnitude Binary (+=0)
enumeration | Sign and Magnitude Binary (+=1)
enumeration | Offset Binary
enumeration | Unsigned Binary
enumeration | IEEE 754 Single Precision
annotation |
documentation
AF
source | <xs:element name="RecordedAnalogFormat" type="TmatsCommon:AnalogRecordedFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>AF</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/InputType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogInputTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Single Ended
enumeration | Differential
annotation |
documentation
AIT
source | <xs:element name="InputType" type="TmatsCommon:AnalogInputTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>AIT</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/Audio

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogAudioType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Audio Present
enumeration | Audio Not Present
annotation |
documentation
AV
source | <xs:element name="Audio" type="TmatsCommon:AnalogAudioType" minOccurs="0"> <xs:annotation> <xs:documentation>AV</xs:documentation> </xs:annotation> </xs:element>

element ChannelType/AudioFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogAudioFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Raw
enumeration | WAV
enumeration | LPCM
enumeration | AC3
enumeration | PreD
enumeration | PstD
enumeration | CvsD
enumeration | Other
annotation |
documentation
AVF
source | <xs:element name="AudioFormat" type="TmatsCommon:AnalogAudioFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>AVF</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy