complexType MeasurementType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
children | TransducerInformation Measurand TelemetryValueDefinition InflightCalibration AmbientValue OtherInformation DataConversion Comments
used by |
element | DataConversionAttributesType/Measurement
attributes |
Name | Type | Use | Default | Fixed | annotation
Name | xs:string | required |  |  |
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="MeasurementType"> <xs:sequence minOccurs="0"> <xs:element name="TransducerInformation" type="TransducerInformationType" minOccurs="0"/> <xs:element name="Measurand" type="MeasurandType" minOccurs="0"/> <xs:element name="TelemetryValueDefinition" type="TelemetryValueDefinitionType" minOccurs="0"/> <xs:element name="InflightCalibration" type="InflightAndAmbientType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeat MC\N times. MC1-n, MC2-n, MC3-n</xs:documentation> </xs:annotation> </xs:element> <xs:element name="AmbientValue" type="InflightAndAmbientType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeat MA\N times. MA1-n, MA2-n, MA3-n</xs:documentation> </xs:annotation> </xs:element> <xs:element name="OtherInformation" type="OtherInformationType" minOccurs="0"/> <xs:element name="DataConversion" type="DataConversionType" minOccurs="0"> <xs:annotation> <xs:documentation>CRT, DCT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute name="Name" type="xs:string" use="required"/> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

attribute MeasurementType/@Name

type | xs:string
properties |
isRef | 0
use | required
source | <xs:attribute name="Name" type="xs:string" use="required"/>

element MeasurementType/TransducerInformation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | TransducerInformationType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Type ModelNumber SerialNumber SecurityClassification OriginationDate RevisionNumber Orientation PointOfContact
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="TransducerInformation" type="TransducerInformationType" minOccurs="0"/>

element MeasurementType/Measurand

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | MeasurandType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Description Alias ExcitationVoltage EngineeringUnits LinkType
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Measurand" type="MeasurandType" minOccurs="0"/>

element MeasurementType/TelemetryValueDefinition

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | TelemetryValueDefinitionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | BinaryFormat FloatingPointFormat BitWeight
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="TelemetryValueDefinition" type="TelemetryValueDefinitionType" minOccurs="0"/>

element MeasurementType/InflightCalibration

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | InflightAndAmbientType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Stimulus TelemetryValue DataValue
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeat MC\N times. MC1-n, MC2-n, MC3-n
source | <xs:element name="InflightCalibration" type="InflightAndAmbientType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeat MC\N times. MC1-n, MC2-n, MC3-n</xs:documentation> </xs:annotation> </xs:element>

element MeasurementType/AmbientValue

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | InflightAndAmbientType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Stimulus TelemetryValue DataValue
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeat MA\N times. MA1-n, MA2-n, MA3-n
source | <xs:element name="AmbientValue" type="InflightAndAmbientType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeat MA\N times. MA1-n, MA2-n, MA3-n</xs:documentation> </xs:annotation> </xs:element>

element MeasurementType/OtherInformation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | OtherInformationType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | MeasurementValue AlertValue WarningValue InitialValue SampleRate
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="OtherInformation" type="OtherInformationType" minOccurs="0"/>

element MeasurementType/DataConversion

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | DataConversionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | PairSets Coefficients NegativePowersOfX Other Derived Discrete PCMTime Time1553 DigitalVoice DigitalVideo
attributes |
Name | Type | Use | Default | Fixed | annotation
DateAndTimeReleased | xs:dateTime | optional |  |  |
Type | TmatsCommon:DataConversionType | required |  |  |
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
CRT, DCT
source | <xs:element name="DataConversion" type="DataConversionType" minOccurs="0"> <xs:annotation> <xs:documentation>CRT, DCT</xs:documentation> </xs:annotation> </xs:element>

element MeasurementType/Comments

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
COM
source | <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy