complexType MessageType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
children | Name Number CommandWordType CommandWordValue Address SpecialProcessing ArincMessageDefinition RTRTReceiveCommandList ModeCode Measurement
used by |
element | Message
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="MessageType"> <xs:sequence minOccurs="0"> <xs:element name="Name" type="xs:string"> <xs:annotation> <xs:documentation>MNA</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Number" type="xs:positiveInteger"> <xs:annotation> <xs:documentation>MID</xs:documentation> </xs:annotation> </xs:element> <xs:element name="CommandWordType" type="TmatsCommon:CommandWordTypeType" default="Address Fields" minOccurs="0"> <xs:annotation> <xs:documentation>CWE</xs:documentation> </xs:annotation> </xs:element> <xs:choice minOccurs="0"> <xs:annotation> <xs:documentation>Depending on CWE value.</xs:documentation> </xs:annotation> <xs:element name="CommandWordValue" type="TmatsCommon:HexType" minOccurs="0"> <xs:annotation> <xs:documentation>CMD</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Address" type="MessageAddressType" minOccurs="0"/> </xs:choice> <xs:element name="SpecialProcessing" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>SPR</xs:documentation> </xs:annotation> </xs:element> <xs:element ref="ArincMessageDefinition" minOccurs="0"> <xs:annotation> <xs:documentation>Only valid, if Bus Type is ARINC 429</xs:documentation> </xs:annotation> </xs:element> <xs:element ref="RTRTReceiveCommandList" minOccurs="0"/> <xs:element ref="ModeCode" minOccurs="0"/> <xs:element ref="Measurement" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element MessageType/Name

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
type | xs:string
properties |
isRef | 0
content | simple
annotation |
documentation
MNA
source | <xs:element name="Name" type="xs:string"> <xs:annotation> <xs:documentation>MNA</xs:documentation> </xs:annotation> </xs:element>

element MessageType/Number

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
content | simple
annotation |
documentation
MID
source | <xs:element name="Number" type="xs:positiveInteger"> <xs:annotation> <xs:documentation>MID</xs:documentation> </xs:annotation> </xs:element>

element MessageType/CommandWordType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
type | TmatsCommon:CommandWordTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Address Fields
facets |
enumeration | Command Word
enumeration | Address Fields
annotation |
documentation
CWE
source | <xs:element name="CommandWordType" type="TmatsCommon:CommandWordTypeType" default="Address Fields" minOccurs="0"> <xs:annotation> <xs:documentation>CWE</xs:documentation> </xs:annotation> </xs:element>

element MessageType/CommandWordValue

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
type | TmatsCommon:HexType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-9|A-F]*
annotation |
documentation
CMD
source | <xs:element name="CommandWordValue" type="TmatsCommon:HexType" minOccurs="0"> <xs:annotation> <xs:documentation>CMD</xs:documentation> </xs:annotation> </xs:element>

element MessageType/Address

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
type | MessageAddressType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | RemoteTerminal SubTerminal TransmitReceiveMode DataWordCountOrModeCode
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Address" type="MessageAddressType" minOccurs="0"/>

element MessageType/SpecialProcessing

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsBGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
SPR
source | <xs:element name="SpecialProcessing" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>SPR</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy