complexType RecordingEventType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | ID Description DataProcessingEnabled Type Priority EventCaptureMode EventInitialCapture LimitCount TriggerMeasurement EventProcessing
used by |
element | RecordingEventDefinitionsType/RecordingEvent
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="RecordingEventType"> <xs:sequence minOccurs="0"> <xs:element name="ID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\ID</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Description" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\D</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataProcessingEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\EDP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Type" type="TmatsCommon:RecordingEventType" default="Recorder" minOccurs="0"> <xs:annotation> <xs:documentation>EV\T</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Priority" type="TmatsCommon:EventPriorityModeType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\P</xs:documentation> </xs:annotation> </xs:element> <xs:element name="EventCaptureMode" type="TmatsCommon:EventCaptureModeType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\CM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="EventInitialCapture" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\IC</xs:documentation> </xs:annotation> </xs:element> <xs:element name="LimitCount" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EV\LC</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TriggerMeasurement" type="TriggerMeasurementType" minOccurs="0"/> <xs:element name="EventProcessing" type="EventProcessingType" minOccurs="0"/> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element RecordingEventType/ID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\ID
source | <xs:element name="ID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\ID</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/Description

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\D
source | <xs:element name="Description" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\D</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/DataProcessingEnabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
EV\EDP
source | <xs:element name="DataProcessingEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\EDP</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/Type

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:RecordingEventType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Recorder
facets |
enumeration | External
enumeration | Measurement Discrete
enumeration | Measurement Limit
enumeration | Recorder
enumeration | Other
annotation |
documentation
EV\T
source | <xs:element name="Type" type="TmatsCommon:RecordingEventType" default="Recorder" minOccurs="0"> <xs:annotation> <xs:documentation>EV\T</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/Priority

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:EventPriorityModeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Priority 1
enumeration | Priority 2
enumeration | Priority 3
enumeration | Priority 4
enumeration | Priority 5
annotation |
documentation
EV\P
source | <xs:element name="Priority" type="TmatsCommon:EventPriorityModeType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\P</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/EventCaptureMode

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:EventCaptureModeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Mode 1
enumeration | Mode 2
enumeration | Mode 3
enumeration | Mode 4
enumeration | Mode 5
enumeration | Mode 6
enumeration | Mode 7
annotation |
documentation
EV\CM
source | <xs:element name="EventCaptureMode" type="TmatsCommon:EventCaptureModeType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\CM</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/EventInitialCapture

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
EV\IC
source | <xs:element name="EventInitialCapture" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>EV\IC</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/LimitCount

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\LC
source | <xs:element name="LimitCount" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EV\LC</xs:documentation> </xs:annotation> </xs:element>

element RecordingEventType/TriggerMeasurement

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TriggerMeasurementType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Source Name
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="TriggerMeasurement" type="TriggerMeasurementType" minOccurs="0"/>

element RecordingEventType/EventProcessing

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | EventProcessingType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DataLink Measurement
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="EventProcessing" type="EventProcessingType" minOccurs="0"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy