complexType EthernetInterfacesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | Name Type IPAddress Ports
used by |
element | RecorderReproducerInfoType/EthernetInterface
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="EthernetInterfacesType"> <xs:sequence> <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EINM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Type" type="TmatsCommon:EthernetType"> <xs:annotation> <xs:documentation>EIT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="IPAddress" type="TmatsCommon:IPAddressType"> <xs:annotation> <xs:documentation>EIIP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Ports" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats EIIP\N times</xs:documentation> </xs:annotation> <xs:complexType> <xs:sequence> <xs:element name="Address"> <xs:annotation> <xs:documentation>EI\PA</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="99999"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="Type" type="TmatsCommon:EthernetType"> <xs:annotation> <xs:documentation>EI\PT</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element EthernetInterfacesType/Name

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EINM
source | <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EINM</xs:documentation> </xs:annotation> </xs:element>

element EthernetInterfacesType/Type

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:EthernetType
properties |
isRef | 0
content | simple
facets |
enumeration | Reserved
enumeration | Download
enumeration | Data Streaming
enumeration | Data Streaming, Download
enumeration | Control and Status
enumeration | Control and Status, Download
enumeration | Control and Status, Data Streaming
enumeration | Control and Status, Data Streaming, Download
annotation |
documentation
EIT
source | <xs:element name="Type" type="TmatsCommon:EthernetType"> <xs:annotation> <xs:documentation>EIT</xs:documentation> </xs:annotation> </xs:element>

element EthernetInterfacesType/IPAddress

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:IPAddressType
properties |
isRef | 0
content | simple
facets |
pattern | (25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)
annotation |
documentation
EIIP
source | <xs:element name="IPAddress" type="TmatsCommon:IPAddressType"> <xs:annotation> <xs:documentation>EIIP</xs:documentation> </xs:annotation> </xs:element>

element EthernetInterfacesType/Ports

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Address Type
annotation |
documentation
Repeats EIIP\N times
source | <xs:element name="Ports" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats EIIP\N times</xs:documentation> </xs:annotation> <xs:complexType> <xs:sequence> <xs:element name="Address"> <xs:annotation> <xs:documentation>EI\PA</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="99999"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="Type" type="TmatsCommon:EthernetType"> <xs:annotation> <xs:documentation>EI\PT</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType> </xs:element>

element EthernetInterfacesType/Ports/Address

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | restriction of xs:nonNegativeInteger
properties |
isRef | 0
content | simple
facets |
minInclusive | 0
maxInclusive | 99999
annotation |
documentation
EI\PA
source | <xs:element name="Address"> <xs:annotation> <xs:documentation>EI\PA</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="99999"/> </xs:restriction> </xs:simpleType> </xs:element>

element EthernetInterfacesType/Ports/Type

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:EthernetType
properties |
isRef | 0
content | simple
facets |
enumeration | Reserved
enumeration | Download
enumeration | Data Streaming
enumeration | Data Streaming, Download
enumeration | Control and Status
enumeration | Control and Status, Download
enumeration | Control and Status, Data Streaming
enumeration | Control and Status, Data Streaming, Download
annotation |
documentation
EI\PT
source | <xs:element name="Type" type="TmatsCommon:EthernetType"> <xs:annotation> <xs:documentation>EI\PT</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy