complexType GroundStationAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsTGroup.xsd
children | IFBandwidth BasebandCompositeBandwidth GainControl FMSystems PMSystems
used by |
element | TransmissionAttributesType/GroundStationAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="GroundStationAttributesType"> <xs:sequence minOccurs="0"> <xs:element name="IFBandwidth" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>GST1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BasebandCompositeBandwidth" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>GST2</xs:documentation> </xs:annotation> </xs:element> <xs:element name="GainControl" type="GainControlType" minOccurs="0"/> <xs:element name="FMSystems" type="FMSystemsType" minOccurs="0"/> <xs:element name="PMSystems" type="PMSystemsType" minOccurs="0"/> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element GroundStationAttributesType/IFBandwidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsTGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
GST1
source | <xs:element name="IFBandwidth" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>GST1</xs:documentation> </xs:annotation> </xs:element>

element GroundStationAttributesType/BasebandCompositeBandwidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsTGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
GST2
source | <xs:element name="BasebandCompositeBandwidth" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>GST2</xs:documentation> </xs:annotation> </xs:element>

element GroundStationAttributesType/GainControl

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsTGroup.xsd
type | GainControlType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | AGCTimeConstant MGCGainSetPoint AFC_APC TrackingBandwidth PolarizationReception
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="GainControl" type="GainControlType" minOccurs="0"/>

element GroundStationAttributesType/FMSystems

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsTGroup.xsd
type | FMSystemsType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | DiscriminatorBandwidth DiscriminatorLinearity
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="FMSystems" type="FMSystemsType" minOccurs="0"/>

element GroundStationAttributesType/PMSystems

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsTGroup.xsd
type | PMSystemsType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | PhaseLockLoopBandwidth
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="PMSystems" type="PMSystemsType" minOccurs="0"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy