simpleType IPAddressType

namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCommonTypes.xsd
type | restriction of xs:string
used by |
element | EthernetInterfacesType/IPAddress
facets |
pattern | (25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)
annotation |
documentation
The IPAddressType data type is an xsd:string of decimal digits separated by '.' (period) characters. It represents the 32-bit dot-decimal notation of IPv4 addresses. Valid IPv4 addresses contain a series of four one-byte long decimal numbers (0 - 255) separated by the '.' character (a total of three '.' characters appear). A valid value of the mdl:IPv4Address data type is "212.23.123.0". See RFC 790 in Section 2.2.2 for further details on IPv4 addresses.
source | <xs:simpleType name="IPAddressType"> <xs:annotation> <xs:documentation>The IPAddressType data type is an xsd:string of decimal digits separated by '.' (period) characters. It represents the 32-bit dot-decimal notation of IPv4 addresses. Valid IPv4 addresses contain a series of four one-byte long decimal numbers (0 - 255) separated by the '.' character (a total of three '.' characters appear). A valid value of the mdl:IPv4Address data type is "212.23.123.0". See RFC 790 in Section 2.2.2 for further details on IPv4 addresses. </xs:documentation> </xs:annotation> <xs:restriction base="xs:string"> <xs:pattern value="(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)\.(25[0-5]|2[0-4][0-9]|[01]?[0-9][0-9]?)"/> </xs:restriction> </xs:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy