complexType SubcommutationType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
children | StartFrame FrameInterval EndFrame
used by |
elements | AsyncEmbeddedFormatType/Subcommutation AsynchronousDataMergeFormatType/Subcommutation
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="SubcommutationType"> <xs:sequence> <xs:element name="StartFrame" type="xs:positiveInteger" default="1" minOccurs="0"/> <xs:element name="FrameInterval" type="xs:nonNegativeInteger" default="1" minOccurs="0"/> <xs:element name="EndFrame" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>If absent, number of frames in PCM format is assumed.</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element SubcommutationType/StartFrame

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 1
source | <xs:element name="StartFrame" type="xs:positiveInteger" default="1" minOccurs="0"/>

element SubcommutationType/FrameInterval

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 1
source | <xs:element name="FrameInterval" type="xs:nonNegativeInteger" default="1" minOccurs="0"/>

element SubcommutationType/EndFrame

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
If absent, number of frames in PCM format is assumed.
source | <xs:element name="EndFrame" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>If absent, number of frames in PCM format is assumed.</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy