complexType ImageDataTypeAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | DataTypeFormat StillImageType DynamicImageFormat TimeStampMode DynamicImageAcquisitionMode ImageFrameRate PreTriggerFrames TotalFrames ExposureTime SensorRotation SensorGain SensorAutoGain SensorWidth SensorHeight MaximumImageWidth MaximumImageHeight ImageWidth ImageHeight ImageOffsetX ImageOffsetY LinePitch BinningHorizontal BinningVertical DecimationHorizontal DecimationVertical ReverseX ReverseY PixelDynamicRangeMinimum PixelDynamicRangeMaximum TestImageType
used by |
element | DataType/ImageDataTypeAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="ImageDataTypeAttributesType"> <xs:sequence minOccurs="0"> <xs:element name="DataTypeFormat" type="TmatsCommon:ImageDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>ITF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="StillImageType" type="TmatsCommon:StillImageTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>SIT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DynamicImageFormat" type="TmatsCommon:DynamicImageFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>DIF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TimeStampMode" type="TmatsCommon:ImageTimeStampModeType" minOccurs="0"> <xs:annotation> <xs:documentation>ITSM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DynamicImageAcquisitionMode" type="TmatsCommon:DynamicImageAcquisitionModeType" minOccurs="0"> <xs:annotation> <xs:documentation>DIAM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ImageFrameRate" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IFR</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PreTriggerFrames" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>PTG</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TotalFrames" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>TOTF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ExposureTime" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>EXP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SensorRotation" minOccurs="0"> <xs:annotation> <xs:documentation>ROT</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="360"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="SensorGain" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>SGV</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SensorAutoGain" type="TmatsCommon:OnOffType" minOccurs="0"> <xs:annotation> <xs:documentation>SAG</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SensorWidth" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ISW</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SensorHeight" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ISH</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MaximumImageWidth" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>MIW</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MaximumImageHeight" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>MIH</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ImageWidth" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IW</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ImageHeight" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IH</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ImageOffsetX" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IOX</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ImageOffsetY" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IOY</xs:documentation> </xs:annotation> </xs:element> <xs:element name="LinePitch" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ILP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BinningHorizontal" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IBH</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BinningVertical" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IBV</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DecimationHorizontal" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDH</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DecimationVertical" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDV</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ReverseX" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>IRX</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ReverseY" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>IRY</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PixelDynamicRangeMinimum" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IPMN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PixelDynamicRangeMaximum" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IPMX</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TestImageType" type="TmatsCommon:TestImageTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>TIT</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element ImageDataTypeAttributesType/DataTypeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:ImageDataTypeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Format 0 (Image)
enumeration | Format 1 (Still Imagery)
enumeration | Format 2 (Dynamic Imagery)
annotation |
documentation
ITF
source | <xs:element name="DataTypeFormat" type="TmatsCommon:ImageDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>ITF</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/StillImageType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:StillImageTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | NITF
enumeration | JPEG
enumeration | JPEG2
enumeration | PNG
annotation |
documentation
SIT
source | <xs:element name="StillImageType" type="TmatsCommon:StillImageTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>SIT</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/DynamicImageFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:DynamicImageFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Mono 8
enumeration | Mono 8 Signed
enumeration | Mono 10
enumeration | Mono 10 Packed
enumeration | Mono 12
enumeration | Mono 12 Packed
enumeration | Mono 14
enumeration | Mono 16
enumeration | Bayer GR8
enumeration | Bayer RG8
enumeration | Bayer GB8
enumeration | Bayer BG8
enumeration | Bayer GR10
enumeration | Bayer RG10
enumeration | Bayer GB10
enumeration | Bayer BG10
enumeration | Bayer GR12
enumeration | Bayer RG12
enumeration | Bayer GB12
enumeration | Bayer BG12
enumeration | Bayer GR10 Packed
enumeration | Bayer RG10 Packed
enumeration | Bayer GB10 Packed
enumeration | Bayer BG10 Packed
enumeration | Bayer GR12 Packed
enumeration | Bayer RG12 Packed
enumeration | Bayer GB12 Packed
enumeration | Bayer BG12 Packed
enumeration | Bayer GR16
enumeration | Bayer RG16
enumeration | Bayer GB16
enumeration | Bayer BG16
enumeration | RGB 8 Packed
enumeration | BGR 8 Packed
enumeration | RGB A8 Packed
enumeration | BGR A8 Packed
enumeration | RGB 10 Packed
enumeration | BGR 10 Packed
enumeration | RGB 12 Packed
enumeration | BGR 12 Packed
enumeration | RGB 16 Packed
enumeration | BGR 16 Packed
enumeration | RGB 10V1 Packed
enumeration | BGR 10V1 Packed
enumeration | RGB 10V2 Packed
enumeration | BGR 10V2 Packed
enumeration | RGB 12V1 Packed
enumeration | RGB 565 Packed
enumeration | BGR 565 Packed
enumeration | YUV 411 Packed
enumeration | YUV 422 Packed
enumeration | YUV 444 Packed
enumeration | YUY V Packed
enumeration | RGB 8 Planar
enumeration | RGB 10 Planar
enumeration | RGB 12 Planar
enumeration | RGB 16 Planar
enumeration | Device Specific
annotation |
documentation
DIF
source | <xs:element name="DynamicImageFormat" type="TmatsCommon:DynamicImageFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>DIF</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/TimeStampMode

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:ImageTimeStampModeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Image Capture Time
enumeration | Image Packetization Time
annotation |
documentation
ITSM
source | <xs:element name="TimeStampMode" type="TmatsCommon:ImageTimeStampModeType" minOccurs="0"> <xs:annotation> <xs:documentation>ITSM</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/DynamicImageAcquisitionMode

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:DynamicImageAcquisitionModeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Single Frame
enumeration | Multi Frame
enumeration | Continuous
annotation |
documentation
DIAM
source | <xs:element name="DynamicImageAcquisitionMode" type="TmatsCommon:DynamicImageAcquisitionModeType" minOccurs="0"> <xs:annotation> <xs:documentation>DIAM</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ImageFrameRate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IFR
source | <xs:element name="ImageFrameRate" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IFR</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/PreTriggerFrames

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
PTG
source | <xs:element name="PreTriggerFrames" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>PTG</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/TotalFrames

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
TOTF
source | <xs:element name="TotalFrames" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>TOTF</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ExposureTime

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:double
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EXP
source | <xs:element name="ExposureTime" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>EXP</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/SensorRotation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | restriction of xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
minInclusive | 0
maxInclusive | 360
annotation |
documentation
ROT
source | <xs:element name="SensorRotation" minOccurs="0"> <xs:annotation> <xs:documentation>ROT</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:nonNegativeInteger"> <xs:minInclusive value="0"/> <xs:maxInclusive value="360"/> </xs:restriction> </xs:simpleType> </xs:element>

element ImageDataTypeAttributesType/SensorGain

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:double
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
SGV
source | <xs:element name="SensorGain" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>SGV</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/SensorAutoGain

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:OnOffType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Off
enumeration | On
annotation |
documentation
SAG
source | <xs:element name="SensorAutoGain" type="TmatsCommon:OnOffType" minOccurs="0"> <xs:annotation> <xs:documentation>SAG</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/SensorWidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ISW
source | <xs:element name="SensorWidth" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ISW</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/SensorHeight

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ISH
source | <xs:element name="SensorHeight" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ISH</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/MaximumImageWidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MIW
source | <xs:element name="MaximumImageWidth" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>MIW</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/MaximumImageHeight

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MIH
source | <xs:element name="MaximumImageHeight" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>MIH</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ImageWidth

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IW
source | <xs:element name="ImageWidth" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IW</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ImageHeight

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IH
source | <xs:element name="ImageHeight" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IH</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ImageOffsetX

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IOX
source | <xs:element name="ImageOffsetX" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IOX</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ImageOffsetY

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IOY
source | <xs:element name="ImageOffsetY" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IOY</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/LinePitch

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ILP
source | <xs:element name="LinePitch" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ILP</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/BinningHorizontal

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IBH
source | <xs:element name="BinningHorizontal" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IBH</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/BinningVertical

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IBV
source | <xs:element name="BinningVertical" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IBV</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/DecimationHorizontal

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IDH
source | <xs:element name="DecimationHorizontal" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDH</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/DecimationVertical

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IDV
source | <xs:element name="DecimationVertical" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDV</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ReverseX

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
IRX
source | <xs:element name="ReverseX" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>IRX</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/ReverseY

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
IRY
source | <xs:element name="ReverseY" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>IRY</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/PixelDynamicRangeMinimum

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IPMN
source | <xs:element name="PixelDynamicRangeMinimum" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IPMN</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/PixelDynamicRangeMaximum

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IPMX
source | <xs:element name="PixelDynamicRangeMaximum" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IPMX</xs:documentation> </xs:annotation> </xs:element>

element ImageDataTypeAttributesType/TestImageType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TestImageTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Off
enumeration | Black
enumeration | White
enumeration | Grey Horizontal Ramp
enumeration | Grey Vertical Ramp
enumeration | Grey Horizontal Ramp Moving
enumeration | Grey Vertical Ramp Moving
enumeration | Horizontal Line Moving
enumeration | Vertical Line Moving
enumeration | Color Bar
enumeration | Frame Counter
enumeration | Device Specific
annotation |
documentation
TIT
source | <xs:element name="TestImageType" type="TmatsCommon:TestImageTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>TIT</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy