complexType AnalogDataTypeAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | DataTypeFormat DataPackingOption SampleRate Channel
used by |
element | DataType/AnalogDataTypeAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="AnalogDataTypeAttributesType"> <xs:sequence minOccurs="0"> <xs:element name="DataTypeFormat" type="TmatsCommon:AnalogDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>ATF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataPackingOption" type="TmatsCommon:AnalogDataPackingOptionType" default="Packed" minOccurs="0"> <xs:annotation> <xs:documentation>ADP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SampleRate" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>ASR</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Channel" type="ChannelType" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element AnalogDataTypeAttributesType/DataTypeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogDataTypeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Format 0 (Reserved)
enumeration | Format 1 (Analog Data)
annotation |
documentation
ATF
source | <xs:element name="DataTypeFormat" type="TmatsCommon:AnalogDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>ATF</xs:documentation> </xs:annotation> </xs:element>

element AnalogDataTypeAttributesType/DataPackingOption

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:AnalogDataPackingOptionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Packed
facets |
enumeration | Packed
enumeration | Unpacked
annotation |
documentation
ADP
source | <xs:element name="DataPackingOption" type="TmatsCommon:AnalogDataPackingOptionType" default="Packed" minOccurs="0"> <xs:annotation> <xs:documentation>ADP</xs:documentation> </xs:annotation> </xs:element>

element AnalogDataTypeAttributesType/SampleRate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:double
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ASR
source | <xs:element name="SampleRate" type="xs:double" minOccurs="0"> <xs:annotation> <xs:documentation>ASR</xs:documentation> </xs:annotation> </xs:element>

element AnalogDataTypeAttributesType/Channel

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | ChannelType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | SubChannelEnabled SubChannelNumber MeasurementName DataLength BitMask MeasurementTransferOrder SampleFactor SampleFilter3dbBandwidth Coupling RecorderInputImpedance InputChannelGain InputFullScaleRange InputOffsetVoltage RecordedAnalogFormat InputType Audio AudioFormat
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Channel" type="ChannelType" minOccurs="0" maxOccurs="unbounded"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy