complexType StreamType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
children | Name Type Layout ElementSize IDLocation Fixed Delimited DataOrientation Message
used by |
element | MessageDataAttributesType/Stream
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="StreamType"> <xs:sequence minOccurs="0"> <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>SNA-i</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Type" type="TmatsCommon:MessageStreamTypeType" default="ASCII" minOccurs="0"> <xs:annotation> <xs:documentation>MDT-i</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Layout" type="TmatsCommon:MessageStreamLayoutType" minOccurs="0"> <xs:annotation> <xs:documentation>MDL-i</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ElementSize" type="xs:nonNegativeInteger" default="8" minOccurs="0"> <xs:annotation> <xs:documentation>MES-i</xs:documentation> </xs:annotation> </xs:element> <xs:element name="IDLocation" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>MIDL-i</xs:documentation> </xs:annotation> </xs:element> <xs:choice> <xs:annotation> <xs:documentation>Depending on value of Layout element</xs:documentation> </xs:annotation> <xs:element name="Fixed" type="FixedType" minOccurs="0"/> <xs:element name="Delimited" type="DelimitedType" minOccurs="0"/> </xs:choice> <xs:element name="DataOrientation" type="TmatsCommon:EndianType" default="Big Endian" minOccurs="0"> <xs:annotation> <xs:documentation>DO-i</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Message" type="MessageType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats NMS\N-i times</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element StreamType/Name

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
SNA-i
source | <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>SNA-i</xs:documentation> </xs:annotation> </xs:element>

element StreamType/Type

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | TmatsCommon:MessageStreamTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | ASCII
facets |
enumeration | ASCII
enumeration | Binary
annotation |
documentation
MDT-i
source | <xs:element name="Type" type="TmatsCommon:MessageStreamTypeType" default="ASCII" minOccurs="0"> <xs:annotation> <xs:documentation>MDT-i</xs:documentation> </xs:annotation> </xs:element>

element StreamType/Layout

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | TmatsCommon:MessageStreamLayoutType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Delimited
enumeration | Fixed
annotation |
documentation
MDL-i
source | <xs:element name="Layout" type="TmatsCommon:MessageStreamLayoutType" minOccurs="0"> <xs:annotation> <xs:documentation>MDL-i</xs:documentation> </xs:annotation> </xs:element>

element StreamType/ElementSize

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 8
annotation |
documentation
MES-i
source | <xs:element name="ElementSize" type="xs:nonNegativeInteger" default="8" minOccurs="0"> <xs:annotation> <xs:documentation>MES-i</xs:documentation> </xs:annotation> </xs:element>

element StreamType/IDLocation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MIDL-i
source | <xs:element name="IDLocation" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>MIDL-i</xs:documentation> </xs:annotation> </xs:element>

element StreamType/Fixed

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | FixedType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Length
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Fixed" type="FixedType" minOccurs="0"/>

element StreamType/Delimited

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | DelimitedType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | MessageDelimiter MessageDelimiterLength FieldDelimiter
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Delimited" type="DelimitedType" minOccurs="0"/>

element StreamType/DataOrientation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | TmatsCommon:EndianType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Big Endian
facets |
enumeration | Big Endian
enumeration | Little Endian
annotation |
documentation
DO-i
source | <xs:element name="DataOrientation" type="TmatsCommon:EndianType" default="Big Endian" minOccurs="0"> <xs:annotation> <xs:documentation>DO-i</xs:documentation> </xs:annotation> </xs:element>

element StreamType/Message

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsSGroup.xsd
type | MessageType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | ID Description Field Measurement
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeats NMS\N-i times
source | <xs:element name="Message" type="MessageType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats NMS\N-i times</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy