complexType DataSourceType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
children | TmatsG:DataSourceSecurityClassification TmatsG:TransmissionAttributes TmatsG:RecorderReproducerAttributes TmatsG:MultiplexModulationGroup TmatsG:DataLink TmatsG:VendorSpecificAttributes
used by |
element | Tmats/DataSource
attributes |
Name | Type | Use | Default | Fixed | annotation
Name | xs:string | optional |  |  |
Type | TmatsCommon:DataSourceType | required |  |  |
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="DataSourceType"> <xs:sequence minOccurs="0"> <xs:element name="DataSourceSecurityClassification" type="TmatsCommon:GeneralSecurityClassificationType" minOccurs="0"> <xs:annotation> <xs:documentation>DSC</xs:documentation> </xs:annotation> </xs:element> <xs:choice> <xs:element name="TransmissionAttributes" type="TmatsT:TransmissionAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS T Group</xs:documentation> </xs:annotation> </xs:element> <xs:element name="RecorderReproducerAttributes" type="TmatsR:RecorderReproducerAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS R Group</xs:documentation> </xs:annotation> </xs:element> </xs:choice> <xs:element name="MultiplexModulationGroup" type="TmatsM:MultiplexModulationGroupType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS M Group</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataLink" type="TmatsG:DataLinkType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Starting point for all DataLink threads</xs:documentation> </xs:annotation> </xs:element> <xs:element name="VendorSpecificAttributes" type="TmatsV:VendorSpecificAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS V-Group</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute name="Name" type="xs:string" use="optional"/> <xs:attribute name="Type" type="TmatsCommon:DataSourceType" use="required"/> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

attribute DataSourceType/@Name

type | xs:string
properties |
isRef | 0
use | optional
source | <xs:attribute name="Name" type="xs:string" use="optional"/>

attribute DataSourceType/@Type

type | TmatsCommon:DataSourceType
properties |
isRef | 0
use | required
facets |
enumeration | RF
enumeration | Tape
enumeration | Storage
enumeration | Distributed Source
enumeration | Direct Source
enumeration | Reproducer
enumeration | Other
source | <xs:attribute name="Type" type="TmatsCommon:DataSourceType" use="required"/>

element DataSourceType/DataSourceSecurityClassification

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsCommon:GeneralSecurityClassificationType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Unclassified
enumeration | Confidential
enumeration | Secret
enumeration | Top Secret
enumeration | Other
annotation |
documentation
DSC
source | <xs:element name="DataSourceSecurityClassification" type="TmatsCommon:GeneralSecurityClassificationType" minOccurs="0"> <xs:annotation> <xs:documentation>DSC</xs:documentation> </xs:annotation> </xs:element>

element DataSourceType/TransmissionAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TransmissionAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | SourceRFAttributes GroundStationAttributes Comments
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS T Group
source | <xs:element name="TransmissionAttributes" type="TmatsT:TransmissionAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS T Group</xs:documentation> </xs:annotation> </xs:element>

element DataSourceType/RecorderReproducerAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | RecorderReproducerAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | ID Description Characteristics RecorderReproducerInfo DataPacket RecordingEventDefinitions Data ReferenceTrack Comments
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS R Group
source | <xs:element name="RecorderReproducerAttributes" type="TmatsR:RecorderReproducerAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS R Group</xs:documentation> </xs:annotation> </xs:element>

element DataSourceType/MultiplexModulationGroup

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | MultiplexModulationGroupType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsM:CompositeSignalStructure TmatsM:BasebandSignal TmatsM:Subcarriers TmatsM:ReferenceChannel TmatsM:DataConversionAttributes TmatsM:Comments
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS M Group
source | <xs:element name="MultiplexModulationGroup" type="TmatsM:MultiplexModulationGroupType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS M Group</xs:documentation> </xs:annotation> </xs:element>

element DataSourceType/DataLink

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsG:DataLinkType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | TmatsG:PCMFormatAttributes TmatsG:BusAttributes TmatsG:MessageDataAttributes TmatsG:DataConversionAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
Name | xs:string | required |  |  |
TmatsVersion |  | optional |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Starting point for all DataLink threads
source | <xs:element name="DataLink" type="TmatsG:DataLinkType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Starting point for all DataLink threads</xs:documentation> </xs:annotation> </xs:element>

element DataSourceType/VendorSpecificAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | VendorSpecificAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
mixed | true
attributes |
Name | Type | Use | Default | Fixed | annotation
Vendor | xs:string | required |  |  |
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS V-Group
source | <xs:element name="VendorSpecificAttributes" type="TmatsV:VendorSpecificAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS V-Group</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy