complexType EventProcessingMeasurementType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | Name PreEventDuration PostEventDuration
used by |
element | EventProcessingType/Measurement
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="EventProcessingMeasurementType"> <xs:sequence minOccurs="0"> <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\PM\MN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PreEventDuration" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EV\PM\PRE</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PostEventDuration" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EV\PM\PST</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element EventProcessingMeasurementType/Name

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\PM\MN
source | <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>EV\PM\MN</xs:documentation> </xs:annotation> </xs:element>

element EventProcessingMeasurementType/PreEventDuration

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\PM\PRE
source | <xs:element name="PreEventDuration" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EV\PM\PRE</xs:documentation> </xs:annotation> </xs:element>

element EventProcessingMeasurementType/PostEventDuration

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EV\PM\PST
source | <xs:element name="PostEventDuration" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EV\PM\PST</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy