complexType AsyncEmbeddedFormatType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
children | DataLinkName Supercom LocationDefinition Location Interval WordLength Mask Subcommutation
used by |
element | PCMFormatAttributesType/AsyncEmbeddedFormat
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="AsyncEmbeddedFormatType"> <xs:sequence> <xs:element name="DataLinkName" type="xs:string"> <xs:annotation> <xs:documentation>AEF\DLN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Supercom" type="TmatsCommon:NonNegativeIntegerOrNo" minOccurs="0"> <xs:annotation> <xs:documentation>AEF1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="LocationDefinition" type="TmatsCommon:PCMLocationDefinitionType" minOccurs="0"> <xs:annotation> <xs:documentation>AEF2</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Location" type="xs:positiveInteger" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF3</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Interval" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AEF4</xs:documentation> </xs:annotation> </xs:element> <xs:element name="WordLength" type="xs:positiveInteger" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF5</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Mask" type="TmatsCommon:BinaryType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF6</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Subcommutation" type="SubcommutationType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF7. If absent, no subcommuation is present. Subcommutation fields include AEF8, AEF9, AEF10</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element AsyncEmbeddedFormatType/DataLinkName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:string
properties |
isRef | 0
content | simple
annotation |
documentation
AEF\DLN
source | <xs:element name="DataLinkName" type="xs:string"> <xs:annotation> <xs:documentation>AEF\DLN</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/Supercom

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | TmatsCommon:NonNegativeIntegerOrNo
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AEF1
source | <xs:element name="Supercom" type="TmatsCommon:NonNegativeIntegerOrNo" minOccurs="0"> <xs:annotation> <xs:documentation>AEF1</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/LocationDefinition

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | TmatsCommon:PCMLocationDefinitionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | First Word And Interval
enumeration | Every Location
enumeration | Contiguous Words
enumeration | Not Applicable
annotation |
documentation
AEF2
source | <xs:element name="LocationDefinition" type="TmatsCommon:PCMLocationDefinitionType" minOccurs="0"> <xs:annotation> <xs:documentation>AEF2</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/Location

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 1
maxOcc | unbounded
content | simple
annotation |
documentation
AEF3
source | <xs:element name="Location" type="xs:positiveInteger" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF3</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/Interval

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
AEF4
source | <xs:element name="Interval" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>AEF4</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/WordLength

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | simple
annotation |
documentation
AEF5
source | <xs:element name="WordLength" type="xs:positiveInteger" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF5</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/Mask

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | TmatsCommon:BinaryType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | simple
facets |
pattern | [0-1]*
annotation |
documentation
AEF6
source | <xs:element name="Mask" type="TmatsCommon:BinaryType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF6</xs:documentation> </xs:annotation> </xs:element>

element AsyncEmbeddedFormatType/Subcommutation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | SubcommutationType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | StartFrame FrameInterval EndFrame
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
AEF7. If absent, no subcommuation is present. Subcommutation fields include AEF8, AEF9, AEF10
source | <xs:element name="Subcommutation" type="SubcommutationType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>AEF7. If absent, no subcommuation is present. Subcommutation fields include AEF8, AEF9, AEF10</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy