complexType Tmats

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
children | TmatsG:ProgramName TmatsG:TestItem TmatsG:TmatsFileName TmatsG:OriginationDate TmatsG:Revision TmatsG:Update TmatsG:TestNumber TmatsG:PointOfContact TmatsG:DataSource TmatsG:TestInformation TmatsG:Checksum TmatsG:Comments TmatsG:AirborneHardwareAttributes
used by |
element | Tmats
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS G-Group
source | <xs:complexType name="Tmats"> <xs:annotation> <xs:documentation>TMATS G-Group</xs:documentation> </xs:annotation> <xs:sequence> <xs:annotation> <xs:documentation>TMATS G Group</xs:documentation> </xs:annotation> <xs:element name="ProgramName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>PN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TestItem" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>TA</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TmatsFileName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>FN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="OriginationDate" type="xs:date" minOccurs="0"> <xs:annotation> <xs:documentation>OD</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Revision" type="TmatsG:RevisionAndUpdateType" minOccurs="0"> <xs:annotation> <xs:documentation>RN and RD</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Update" type="TmatsG:RevisionAndUpdateType" minOccurs="0"> <xs:annotation> <xs:documentation>UN and UD</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TestNumber" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>TN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PointOfContact" type="TmatsCommon:PointOfContactType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>POC1, POC2, POC3, POC4</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataSource" type="TmatsG:DataSourceType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>DSI, DST</xs:documentation> </xs:annotation> <xs:key name="DataLinkKey"> <xs:selector xpath="TmatsG:DataLink"/> <xs:field xpath="@Name"/> </xs:key> <xs:keyref name="ChannelDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data"/> <xs:field xpath="TmatsR:ChannelDataLinkName"/> </xs:keyref> <xs:keyref name="ARINC429BusDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:ARINC429BusDataTypeAttributes/TmatsR:SubChannel"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="UARTDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:UARTDataTypeAttributes/TmatsR:SubChannel"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="MessageDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:MessageDataTypeAttributes/TmatsR:SubChannel"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="EthernetDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:EthernetDataTypeAttributes/TmatsR:Network"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="BaseBandSignalDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:MultiplexModulationGroup/TmatsM:BasebandSignal"/> <xs:field xpath="TmatsM:DataLinkName"/> </xs:keyref> <xs:keyref name="IRIGSubcarrierDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:MultiplexModulationGroup/TmatsM:Subcarriers/TmatsM:IRIGSubcarrier"/> <xs:field xpath="TmatsM:DataLinkName"/> </xs:keyref> <xs:keyref name="AsyncEmbeddedFormatDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:DataLink/TmatsG:PCMFormatAttributes/TmatsP:AsyncEmbeddedFormat"/> <xs:field xpath="TmatsP:DataLinkName"/> </xs:keyref> <xs:keyref name="FormatStructureChangeDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:DataLink/TmatsG:PCMFormatAttributes/TmatsP:FormatChange/TmatsP:FormatStructureChange"/> <xs:field xpath="TmatsP:DataLinkName"/> </xs:keyref> </xs:element> <xs:element name="TestInformation" type="TmatsG:TestInformationType" minOccurs="0"/> <xs:element name="Checksum" type="TmatsG:ChecksumType" minOccurs="0"> <xs:annotation> <xs:documentation>SHA - Added in 106-15</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="AirborneHardwareAttributes" type="TmatsH:AirborneHardwareAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS H-Group</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion" use="required"/> </xs:complexType>

element Tmats/ProgramName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
PN
source | <xs:element name="ProgramName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>PN</xs:documentation> </xs:annotation> </xs:element>

element Tmats/TestItem

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
TA
source | <xs:element name="TestItem" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>TA</xs:documentation> </xs:annotation> </xs:element>

element Tmats/TmatsFileName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
FN
source | <xs:element name="TmatsFileName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>FN</xs:documentation> </xs:annotation> </xs:element>

element Tmats/OriginationDate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | xs:date
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
OD
source | <xs:element name="OriginationDate" type="xs:date" minOccurs="0"> <xs:annotation> <xs:documentation>OD</xs:documentation> </xs:annotation> </xs:element>

element Tmats/Revision

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsG:RevisionAndUpdateType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsG:Number TmatsG:Date
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
RN and RD
source | <xs:element name="Revision" type="TmatsG:RevisionAndUpdateType" minOccurs="0"> <xs:annotation> <xs:documentation>RN and RD</xs:documentation> </xs:annotation> </xs:element>

element Tmats/Update

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsG:RevisionAndUpdateType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsG:Number TmatsG:Date
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
UN and UD
source | <xs:element name="Update" type="TmatsG:RevisionAndUpdateType" minOccurs="0"> <xs:annotation> <xs:documentation>UN and UD</xs:documentation> </xs:annotation> </xs:element>

element Tmats/TestNumber

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
TN
source | <xs:element name="TestNumber" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>TN</xs:documentation> </xs:annotation> </xs:element>

element Tmats/PointOfContact

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsCommon:PointOfContactType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Name Agency Address Telephone
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
POC1, POC2, POC3, POC4
source | <xs:element name="PointOfContact" type="TmatsCommon:PointOfContactType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>POC1, POC2, POC3, POC4</xs:documentation> </xs:annotation> </xs:element>

element Tmats/DataSource

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsG:DataSourceType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | TmatsG:DataSourceSecurityClassification TmatsG:TransmissionAttributes TmatsG:RecorderReproducerAttributes TmatsG:MultiplexModulationGroup TmatsG:DataLink TmatsG:VendorSpecificAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
Name | xs:string | optional |  |  |
Type | TmatsCommon:DataSourceType | required |  |  |
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
identity constraints |
| Name | Refer | Selector | Field(s)
key | DataLinkKey |  | TmatsG:DataLink | @Name
keyref | ChannelDataLinkRef | TmatsG:DataLinkKey | TmatsG:RecorderReproducerAttributes/TmatsR:Data | TmatsR:ChannelDataLinkName
keyref | ARINC429BusDataTypeRef | TmatsG:DataLinkKey | TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:ARINC429BusDataTypeAttributes/TmatsR:SubChannel | TmatsR:Name
keyref | UARTDataTypeRef | TmatsG:DataLinkKey | TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:UARTDataTypeAttributes/TmatsR:SubChannel | TmatsR:Name
keyref | MessageDataTypeRef | TmatsG:DataLinkKey | TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:MessageDataTypeAttributes/TmatsR:SubChannel | TmatsR:Name
keyref | EthernetDataTypeRef | TmatsG:DataLinkKey | TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:EthernetDataTypeAttributes/TmatsR:Network | TmatsR:Name
keyref | BaseBandSignalDataLinkRef | TmatsG:DataLinkKey | TmatsG:MultiplexModulationGroup/TmatsM:BasebandSignal | TmatsM:DataLinkName
keyref | IRIGSubcarrierDataLinkRef | TmatsG:DataLinkKey | TmatsG:MultiplexModulationGroup/TmatsM:Subcarriers/TmatsM:IRIGSubcarrier | TmatsM:DataLinkName
keyref | AsyncEmbeddedFormatDataLinkRef | TmatsG:DataLinkKey | TmatsG:DataLink/TmatsG:PCMFormatAttributes/TmatsP:AsyncEmbeddedFormat | TmatsP:DataLinkName
keyref | FormatStructureChangeDataLinkRef | TmatsG:DataLinkKey | TmatsG:DataLink/TmatsG:PCMFormatAttributes/TmatsP:FormatChange/TmatsP:FormatStructureChange | TmatsP:DataLinkName
annotation |
documentation
DSI, DST
source | <xs:element name="DataSource" type="TmatsG:DataSourceType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>DSI, DST</xs:documentation> </xs:annotation> <xs:key name="DataLinkKey"> <xs:selector xpath="TmatsG:DataLink"/> <xs:field xpath="@Name"/> </xs:key> <xs:keyref name="ChannelDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data"/> <xs:field xpath="TmatsR:ChannelDataLinkName"/> </xs:keyref> <xs:keyref name="ARINC429BusDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:ARINC429BusDataTypeAttributes/TmatsR:SubChannel"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="UARTDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:UARTDataTypeAttributes/TmatsR:SubChannel"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="MessageDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:MessageDataTypeAttributes/TmatsR:SubChannel"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="EthernetDataTypeRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:RecorderReproducerAttributes/TmatsR:Data/TmatsR:EthernetDataTypeAttributes/TmatsR:Network"/> <xs:field xpath="TmatsR:Name"/> </xs:keyref> <xs:keyref name="BaseBandSignalDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:MultiplexModulationGroup/TmatsM:BasebandSignal"/> <xs:field xpath="TmatsM:DataLinkName"/> </xs:keyref> <xs:keyref name="IRIGSubcarrierDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:MultiplexModulationGroup/TmatsM:Subcarriers/TmatsM:IRIGSubcarrier"/> <xs:field xpath="TmatsM:DataLinkName"/> </xs:keyref> <xs:keyref name="AsyncEmbeddedFormatDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:DataLink/TmatsG:PCMFormatAttributes/TmatsP:AsyncEmbeddedFormat"/> <xs:field xpath="TmatsP:DataLinkName"/> </xs:keyref> <xs:keyref name="FormatStructureChangeDataLinkRef" refer="TmatsG:DataLinkKey"> <xs:selector xpath="TmatsG:DataLink/TmatsG:PCMFormatAttributes/TmatsP:FormatChange/TmatsP:FormatStructureChange"/> <xs:field xpath="TmatsP:DataLinkName"/> </xs:keyref> </xs:element>

element Tmats/TestInformation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsG:TestInformationType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsG:Duration TmatsG:PreTestRequirement TmatsG:PostTestRequirement TmatsG:SecurityClassification
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="TestInformation" type="TmatsG:TestInformationType" minOccurs="0"/>

element Tmats/Checksum

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsG:ChecksumType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-9]-[0-9A-Fa-f]{64}
annotation |
documentation
SHA - Added in 106-15
source | <xs:element name="Checksum" type="TmatsG:ChecksumType" minOccurs="0"> <xs:annotation> <xs:documentation>SHA - Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

element Tmats/Comments

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
COM
source | <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element>

element Tmats/AirborneHardwareAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsGGroup.xsd
type | TmatsH:AirborneHardwareAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
mixed | true
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS H-Group
source | <xs:element name="AirborneHardwareAttributes" type="TmatsH:AirborneHardwareAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>TMATS H-Group</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy