complexType RecordingIndexType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | Enabled ChannelID Type TimeValue CountValue
used by |
element | RecordingEventDefinitionsType/RecordingIndex
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="RecordingIndexType"> <xs:sequence minOccurs="0"> <xs:element name="Enabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\E</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ChannelID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\TK1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Type" type="TmatsCommon:RecordingIndexTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\IT</xs:documentation> </xs:annotation> </xs:element> <xs:choice minOccurs="0"> <xs:annotation> <xs:documentation>Depending on value of Type</xs:documentation> </xs:annotation> <xs:element name="TimeValue" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\ITV</xs:documentation> </xs:annotation> </xs:element> <xs:element name="CountValue" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\ICV</xs:documentation> </xs:annotation> </xs:element> </xs:choice> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element RecordingIndexType/Enabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
IDX\E
source | <xs:element name="Enabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\E</xs:documentation> </xs:annotation> </xs:element>

element RecordingIndexType/ChannelID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IDX\TK1
source | <xs:element name="ChannelID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\TK1</xs:documentation> </xs:annotation> </xs:element>

element RecordingIndexType/Type

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:RecordingIndexTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Time
enumeration | Count
annotation |
documentation
IDX\IT
source | <xs:element name="Type" type="TmatsCommon:RecordingIndexTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\IT</xs:documentation> </xs:annotation> </xs:element>

element RecordingIndexType/TimeValue

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IDX\ITV
source | <xs:element name="TimeValue" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\ITV</xs:documentation> </xs:annotation> </xs:element>

element RecordingIndexType/CountValue

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
IDX\ICV
source | <xs:element name="CountValue" type="xs:nonNegativeInteger" minOccurs="0"> <xs:annotation> <xs:documentation>IDX\ICV</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy