complexType TelemetryOutputAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | OutputStreamName StreamID ConfigurationPacketHashCodeRate ConfigurationPacketRate
used by |
element | DataType/TelemetryOutputAttributes
annotation |
documentation
Added in 106-15
source | <xs:complexType name="TelemetryOutputAttributesType"> <xs:annotation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> <xs:all> <xs:element name="OutputStreamName" type="OutputStreamNameType"> <xs:annotation> <xs:documentation>R-x\OSNM-n</xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element> <xs:element name="StreamID" type="OutputStreamIDType" default="0" minOccurs="0"> <xs:annotation> <xs:documentation>R-x\SID-n</xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ConfigurationPacketHashCodeRate" type="PacketRateType" default="Disabled" minOccurs="0"> <xs:annotation> <xs:documentation>R-x\HRATE-n</xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ConfigurationPacketRate" type="PacketRateType" default="Disabled" minOccurs="0"> <xs:annotation> <xs:documentation>R-x\CRATE-n </xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element> </xs:all> </xs:complexType>

element TelemetryOutputAttributesType/OutputStreamName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | OutputStreamNameType
properties |
isRef | 0
content | simple
facets |
maxLength | 32
annotation |
documentation
R-x\OSNM-n
documentation
Added in 106-15
source | <xs:element name="OutputStreamName" type="OutputStreamNameType"> <xs:annotation> <xs:documentation>R-x\OSNM-n</xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

element TelemetryOutputAttributesType/StreamID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | OutputStreamIDType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 0
facets |
minInclusive | 0
maxInclusive | 15
annotation |
documentation
R-x\SID-n
documentation
Added in 106-15
source | <xs:element name="StreamID" type="OutputStreamIDType" default="0" minOccurs="0"> <xs:annotation> <xs:documentation>R-x\SID-n</xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

element TelemetryOutputAttributesType/ConfigurationPacketHashCodeRate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | PacketRateType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Disabled
annotation |
documentation
R-x\HRATE-n
documentation
Added in 106-15
source | <xs:element name="ConfigurationPacketHashCodeRate" type="PacketRateType" default="Disabled" minOccurs="0"> <xs:annotation> <xs:documentation>R-x\HRATE-n</xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

element TelemetryOutputAttributesType/ConfigurationPacketRate

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | PacketRateType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Disabled
annotation |
documentation
R-x\CRATE-n
documentation
Added in 106-15
source | <xs:element name="ConfigurationPacketRate" type="PacketRateType" default="Disabled" minOccurs="0"> <xs:annotation> <xs:documentation>R-x\CRATE-n </xs:documentation> <xs:documentation>Added in 106-15</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy