complexType RTRTType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | CommandWordEntry CommandWord Address
used by |
element | MessageFilteringDefinitionsType/RTRT
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="RTRTType"> <xs:sequence minOccurs="0"> <xs:element name="CommandWordEntry" type="TmatsCommon:CommandWordTypeType" default="Address Fields" minOccurs="0"> <xs:annotation> <xs:documentation>RCWE</xs:documentation> </xs:annotation> </xs:element> <xs:choice minOccurs="0"> <xs:annotation> <xs:documentation>Depending on RCWE value.</xs:documentation> </xs:annotation> <xs:element name="CommandWord" type="TmatsCommon:HexType" minOccurs="0"> <xs:annotation> <xs:documentation>RCMD</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Address" type="RTRTAddressType" minOccurs="0"/> </xs:choice> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element RTRTType/CommandWordEntry

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:CommandWordTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Address Fields
facets |
enumeration | Command Word
enumeration | Address Fields
annotation |
documentation
RCWE
source | <xs:element name="CommandWordEntry" type="TmatsCommon:CommandWordTypeType" default="Address Fields" minOccurs="0"> <xs:annotation> <xs:documentation>RCWE</xs:documentation> </xs:annotation> </xs:element>

element RTRTType/CommandWord

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:HexType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-9|A-F]*
annotation |
documentation
RCMD
source | <xs:element name="CommandWord" type="TmatsCommon:HexType" minOccurs="0"> <xs:annotation> <xs:documentation>RCMD</xs:documentation> </xs:annotation> </xs:element>

element RTRTType/Address

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | RTRTAddressType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | RemoteTerminalAddress SubTerminalAddress DataWordCount
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Address" type="RTRTAddressType" minOccurs="0"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy