complexType AddressType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | RemoteTerminalAddress TransmitReceiveMode SubTerminalAddress DataWordCountOrModeCode
used by |
element | MessageFilteringDefinitionsType/Address
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="AddressType"> <xs:sequence> <xs:element name="RemoteTerminalAddress" type="TmatsCommon:BinaryWithDontCareType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\TRA</xs:documentation> </xs:annotation> </xs:element> <xs:element name="TransmitReceiveMode" type="TmatsCommon:TransmitReceiveModeType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\TRM</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SubTerminalAddress" type="TmatsCommon:BinaryWithDontCareType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\STA</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataWordCountOrModeCode" type="TmatsCommon:BinaryWithDontCareType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\DWC</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element AddressType/RemoteTerminalAddress

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:BinaryWithDontCareType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-1|X]*
annotation |
documentation
MFD\TRA
source | <xs:element name="RemoteTerminalAddress" type="TmatsCommon:BinaryWithDontCareType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\TRA</xs:documentation> </xs:annotation> </xs:element>

element AddressType/TransmitReceiveMode

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TransmitReceiveModeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Transmit
enumeration | Receive
annotation |
documentation
MFD\TRM
source | <xs:element name="TransmitReceiveMode" type="TmatsCommon:TransmitReceiveModeType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\TRM</xs:documentation> </xs:annotation> </xs:element>

element AddressType/SubTerminalAddress

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:BinaryWithDontCareType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-1|X]*
annotation |
documentation
MFD\STA
source | <xs:element name="SubTerminalAddress" type="TmatsCommon:BinaryWithDontCareType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\STA</xs:documentation> </xs:annotation> </xs:element>

element AddressType/DataWordCountOrModeCode

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:BinaryWithDontCareType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
pattern | [0-1|X]*
annotation |
documentation
MFD\DWC
source | <xs:element name="DataWordCountOrModeCode" type="TmatsCommon:BinaryWithDontCareType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\DWC</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy