complexType MIL-STD-1553BusDataTypeAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | BusDataTypeFormat FilteringEnabled PostProcessOverwriteAndFilteringEnabled MessageFilteringType MessageFilteringDefinitions MeasurementOverwriteDefinitions
used by |
element | DataType/MIL-STD-1553BusDataTypeAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="MIL-STD-1553BusDataTypeAttributesType"> <xs:sequence minOccurs="0"> <xs:element name="BusDataTypeFormat" type="TmatsCommon:BusDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>BTF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="FilteringEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>MRF\E</xs:documentation> </xs:annotation> </xs:element> <xs:element name="PostProcessOverwriteAndFilteringEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>MOF\T</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MessageFilteringType" type="TmatsCommon:FilterType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\FDT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MessageFilteringDefinitions" type="MessageFilteringDefinitionsType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats MFD\N times</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MeasurementOverwriteDefinitions" type="MeasurementOverwriteType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>BME\SMN and BME\MFOT. Repeat BME\N times</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element MIL-STD-1553BusDataTypeAttributesType/BusDataTypeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:BusDataTypeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Format 0 (Reserved)
enumeration | Format 1 (MIL-STD-1553B Data)
enumeration | Format 2 (16PP194 Bus)
annotation |
documentation
BTF
source | <xs:element name="BusDataTypeFormat" type="TmatsCommon:BusDataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>BTF</xs:documentation> </xs:annotation> </xs:element>

element MIL-STD-1553BusDataTypeAttributesType/FilteringEnabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
MRF\E
source | <xs:element name="FilteringEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>MRF\E</xs:documentation> </xs:annotation> </xs:element>

element MIL-STD-1553BusDataTypeAttributesType/PostProcessOverwriteAndFilteringEnabled

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:TrueFalseType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | True
enumeration | False
annotation |
documentation
MOF\T
source | <xs:element name="PostProcessOverwriteAndFilteringEnabled" type="TmatsCommon:TrueFalseType" minOccurs="0"> <xs:annotation> <xs:documentation>MOF\T</xs:documentation> </xs:annotation> </xs:element>

element MIL-STD-1553BusDataTypeAttributesType/MessageFilteringType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:FilterType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Inclusive Filtering
enumeration | Exclusive Filtering
annotation |
documentation
MFD\FDT
source | <xs:element name="MessageFilteringType" type="TmatsCommon:FilterType" minOccurs="0"> <xs:annotation> <xs:documentation>MFD\FDT</xs:documentation> </xs:annotation> </xs:element>

element MIL-STD-1553BusDataTypeAttributesType/MessageFilteringDefinitions

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | MessageFilteringDefinitionsType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | MessageNumber Type CommandWordEntry CommandWord Address RTRT
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeats MFD\N times
source | <xs:element name="MessageFilteringDefinitions" type="MessageFilteringDefinitionsType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats MFD\N times</xs:documentation> </xs:annotation> </xs:element>

element MIL-STD-1553BusDataTypeAttributesType/MeasurementOverwriteDefinitions

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | MeasurementOverwriteType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Measurement OverwriteTag
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
BME\SMN and BME\MFOT. Repeat BME\N times
source | <xs:element name="MeasurementOverwriteDefinitions" type="MeasurementOverwriteType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>BME\SMN and BME\MFOT. Repeat BME\N times</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy