complexType ARINC429BusDataTypeAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | DataTypeFormat SubChannel
used by |
element | DataType/ARINC429BusDataTypeAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="ARINC429BusDataTypeAttributesType"> <xs:sequence minOccurs="0"> <xs:element name="DataTypeFormat" type="TmatsCommon:Arinc429DataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>ABTF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="SubChannel" type="ARINCSubChannelType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats NAS\N times</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element ARINC429BusDataTypeAttributesType/DataTypeFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | TmatsCommon:Arinc429DataTypeFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Format 0 (ARINC 429 Data)
enumeration | Format 1 (Reserved)
annotation |
documentation
ABTF
source | <xs:element name="DataTypeFormat" type="TmatsCommon:Arinc429DataTypeFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>ABTF</xs:documentation> </xs:annotation> </xs:element>

element ARINC429BusDataTypeAttributesType/SubChannel

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | ARINCSubChannelType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | Number Name
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeats NAS\N times
source | <xs:element name="SubChannel" type="ARINCSubChannelType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats NAS\N times</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy