complexType MeasurementFragmentsType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
children | FragmentPosition FragmentTransferOrder StartWord WordInterval EndWord StartFrame FrameInterval EndFrame BitMask
used by |
element | MeasurementLocationType/MeasurementFragments
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="MeasurementFragmentsType"> <xs:sequence> <xs:element name="FragmentPosition" default="1" minOccurs="0"> <xs:annotation> <xs:documentation>WFP</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:positiveInteger"> <xs:maxInclusive value="8"/> </xs:restriction> </xs:simpleType> </xs:element> <xs:element name="FragmentTransferOrder" type="TmatsCommon:TransferOrderType" default="Default" minOccurs="0"> <xs:annotation> <xs:documentation>WFT</xs:documentation> </xs:annotation> </xs:element> <xs:element name="StartWord" type="xs:positiveInteger"> <xs:annotation> <xs:documentation>WP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="WordInterval" type="xs:nonNegativeInteger" default="0" minOccurs="0"> <xs:annotation> <xs:documentation>WI</xs:documentation> </xs:annotation> </xs:element> <xs:element name="EndWord" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EWP (If absent, assume "end of frame", and is only valid if WordInterval is present, and greater than 0)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="StartFrame" type="xs:positiveInteger" default="1" minOccurs="0"> <xs:annotation> <xs:documentation>FP</xs:documentation> </xs:annotation> </xs:element> <xs:element name="FrameInterval" type="xs:nonNegativeInteger" default="0" minOccurs="0"> <xs:annotation> <xs:documentation>FI</xs:documentation> </xs:annotation> </xs:element> <xs:element name="EndFrame" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EFP (If absent, assume "end of major frame", and is only valid if FrameInterval is present, and greater than 0)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BitMask" type="TmatsCommon:MeasurementBitMaskType" default="Full Word" minOccurs="0"> <xs:annotation> <xs:documentation>WFM</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element MeasurementFragmentsType/FragmentPosition

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | restriction of xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 1
facets |
maxInclusive | 8
annotation |
documentation
WFP
source | <xs:element name="FragmentPosition" default="1" minOccurs="0"> <xs:annotation> <xs:documentation>WFP</xs:documentation> </xs:annotation> <xs:simpleType> <xs:restriction base="xs:positiveInteger"> <xs:maxInclusive value="8"/> </xs:restriction> </xs:simpleType> </xs:element>

element MeasurementFragmentsType/FragmentTransferOrder

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | TmatsCommon:TransferOrderType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Default
annotation |
documentation
WFT
source | <xs:element name="FragmentTransferOrder" type="TmatsCommon:TransferOrderType" default="Default" minOccurs="0"> <xs:annotation> <xs:documentation>WFT</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/StartWord

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
content | simple
annotation |
documentation
WP
source | <xs:element name="StartWord" type="xs:positiveInteger"> <xs:annotation> <xs:documentation>WP</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/WordInterval

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 0
annotation |
documentation
WI
source | <xs:element name="WordInterval" type="xs:nonNegativeInteger" default="0" minOccurs="0"> <xs:annotation> <xs:documentation>WI</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/EndWord

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EWP (If absent, assume "end of frame", and is only valid if WordInterval is present, and greater than 0)
source | <xs:element name="EndWord" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EWP (If absent, assume "end of frame", and is only valid if WordInterval is present, and greater than 0)</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/StartFrame

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 1
annotation |
documentation
FP
source | <xs:element name="StartFrame" type="xs:positiveInteger" default="1" minOccurs="0"> <xs:annotation> <xs:documentation>FP</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/FrameInterval

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | xs:nonNegativeInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | 0
annotation |
documentation
FI
source | <xs:element name="FrameInterval" type="xs:nonNegativeInteger" default="0" minOccurs="0"> <xs:annotation> <xs:documentation>FI</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/EndFrame

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
EFP (If absent, assume "end of major frame", and is only valid if FrameInterval is present, and greater than 0)
source | <xs:element name="EndFrame" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>EFP (If absent, assume "end of major frame", and is only valid if FrameInterval is present, and greater than 0)</xs:documentation> </xs:annotation> </xs:element>

element MeasurementFragmentsType/BitMask

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsDGroup.xsd
type | TmatsCommon:MeasurementBitMaskType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | Full Word
facets |
pattern | [0-1]*
pattern | Full Word
annotation |
documentation
WFM
source | <xs:element name="BitMask" type="TmatsCommon:MeasurementBitMaskType" default="Full Word" minOccurs="0"> <xs:annotation> <xs:documentation>WFM</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy