complexType RecorderReproducerAttributesType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
children | ID Description Characteristics RecorderReproducerInfo DataPacket RecordingEventDefinitions Data ReferenceTrack Comments
used by |
element | DataSourceType/RecorderReproducerAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS R-Group
source | <xs:complexType name="RecorderReproducerAttributesType"> <xs:annotation> <xs:documentation>TMATS R-Group</xs:documentation> </xs:annotation> <xs:sequence minOccurs="0"> <xs:element name="ID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>RID</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Description" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>R1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Characteristics" type="CharacteristicsType" minOccurs="0"/> <xs:element name="RecorderReproducerInfo" type="RecorderReproducerInfoType" minOccurs="0"/> <xs:element name="DataPacket" type="DataPacketType" minOccurs="0"/> <xs:element name="RecordingEventDefinitions" type="RecordingEventDefinitionsType" minOccurs="0"/> <xs:element name="Data" type="DataType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeat N times</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ReferenceTrack" type="ReferenceTrackType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats RT\N times</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion" use="required"/> </xs:complexType>

element RecorderReproducerAttributesType/ID

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
RID
source | <xs:element name="ID" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>RID</xs:documentation> </xs:annotation> </xs:element>

element RecorderReproducerAttributesType/Description

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
R1
source | <xs:element name="Description" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>R1</xs:documentation> </xs:annotation> </xs:element>

element RecorderReproducerAttributesType/Characteristics

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | CharacteristicsType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Type Manufacturer Code MediaLocation ExternalRMMBusSpeed Width Housing TypeOfTracks NumberOfTracksOrChannels RecordSpeed DataPackingDensity Rewound NumberOfSourceBits
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Characteristics" type="CharacteristicsType" minOccurs="0"/>

element RecorderReproducerAttributesType/RecorderReproducerInfo

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | RecorderReproducerInfoType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Manufacturer Model OriginalRecording OriginalRecordingDateAndTime CreatingOrganizationPointOfContact DateAndTimeOfCopy CopyingOrganizationPointOfContact PostProcessModifiedRecording PostProcessModificationType DateAndTimeOfModification ModifyingOrganizationPOC ContinuousRecordingEnabled SetupSource SerialNumber FirmwareRevision Module RMM EthernetInterface ChannelGroup DrivesAndVolumes StreamDriveVolumeLinks
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="RecorderReproducerInfo" type="RecorderReproducerInfoType" minOccurs="0"/>

element RecorderReproducerAttributesType/DataPacket

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | DataPacketType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | UserDefinedChannelID
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="DataPacket" type="DataPacketType" minOccurs="0"/>

element RecorderReproducerAttributesType/RecordingEventDefinitions

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | RecordingEventDefinitionsType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Enabled ChannelID InternalEventsEnabled RecordingEvent RecordingIndex RecorderControl
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="RecordingEventDefinitions" type="RecordingEventDefinitionsType" minOccurs="0"/>

element RecorderReproducerAttributesType/Data

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | DataType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | TrackNumberOrChannelID RecordingTechnique InputStreamDerandomized DataSourceID DataDirection RecorderPhysicalChannelNumber ChannelEnable ChannelDataType ChannelDataLinkName SecondaryHeaderTimeFormat PCMDataTypeAttributes MIL-STD-1553BusDataTypeAttributes AnalogDataTypeAttributes DiscreteDataTypeAttributes ARINC429BusDataTypeAttributes VideoDataTypeAttributes TimeDataTypeAttributes ImageDataTypeAttributes UARTDataTypeAttributes MessageDataTypeAttributes IEEE1394DataTypeAttributes ParallelDataTypeAttributes EthernetDataTypeAttributes TSPICTSDataTypeAttributes CanBusDataTypeAttributes FibreChannelDataTypeAttributes TelemetryOutputAttributes
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeat N times
source | <xs:element name="Data" type="DataType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeat N times</xs:documentation> </xs:annotation> </xs:element>

element RecorderReproducerAttributesType/ReferenceTrack

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | ReferenceTrackType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | TrackNumber ReferenceFrequency
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Repeats RT\N times
source | <xs:element name="ReferenceTrack" type="ReferenceTrackType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Repeats RT\N times</xs:documentation> </xs:annotation> </xs:element>

element RecorderReproducerAttributesType/Comments

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsRGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
COM
source | <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy