complexType BasebandSignalType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
children | TmatsM:SignalType TmatsM:LowPassFilter TmatsM:DataLinkName TmatsM:MeasurementName
used by |
element | MultiplexModulationGroupType/BasebandSignal
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="BasebandSignalType"> <xs:sequence minOccurs="0"> <xs:element name="SignalType" type="TmatsCommon:BasebandSignalTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>BSG1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="LowPassFilter" type="TmatsM:LowPassFilterType" minOccurs="0"> <xs:annotation> <xs:documentation>BSF1 and BSF2</xs:documentation> </xs:annotation> </xs:element> <xs:choice minOccurs="0"> <xs:annotation> <xs:documentation>Based upon value of BSG1</xs:documentation> </xs:annotation> <xs:element name="DataLinkName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>BB\DLN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MeasurementName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>BB\MN</xs:documentation> </xs:annotation> </xs:element> </xs:choice> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element BasebandSignalType/SignalType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | TmatsCommon:BasebandSignalTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
BSG1
source | <xs:element name="SignalType" type="TmatsCommon:BasebandSignalTypeType" minOccurs="0"> <xs:annotation> <xs:documentation>BSG1</xs:documentation> </xs:annotation> </xs:element>

element BasebandSignalType/LowPassFilter

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | LowPassFilterType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsM:Bandwidth TmatsM:Type
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
BSF1 and BSF2
source | <xs:element name="LowPassFilter" type="TmatsM:LowPassFilterType" minOccurs="0"> <xs:annotation> <xs:documentation>BSF1 and BSF2</xs:documentation> </xs:annotation> </xs:element>

element BasebandSignalType/DataLinkName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
BB\DLN
source | <xs:element name="DataLinkName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>BB\DLN</xs:documentation> </xs:annotation> </xs:element>

element BasebandSignalType/MeasurementName

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
BB\MN
source | <xs:element name="MeasurementName" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>BB\MN</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy