complexType MeasurandType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
children | Description Alias ExcitationVoltage EngineeringUnits LinkType
used by |
element | MeasurementType/Measurand
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="MeasurandType"> <xs:sequence minOccurs="0"> <xs:element name="Description" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MN1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Alias" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MNA</xs:documentation> </xs:annotation> </xs:element> <xs:element name="ExcitationVoltage" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MN2</xs:documentation> </xs:annotation> </xs:element> <xs:element name="EngineeringUnits" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MN3</xs:documentation> </xs:annotation> </xs:element> <xs:element name="LinkType" type="TmatsCommon:LinkTypeType" default="PCM" minOccurs="0"> <xs:annotation> <xs:documentation>MN4</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element MeasurandType/Description

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MN1
source | <xs:element name="Description" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MN1</xs:documentation> </xs:annotation> </xs:element>

element MeasurandType/Alias

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MNA
source | <xs:element name="Alias" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MNA</xs:documentation> </xs:annotation> </xs:element>

element MeasurandType/ExcitationVoltage

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MN2
source | <xs:element name="ExcitationVoltage" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MN2</xs:documentation> </xs:annotation> </xs:element>

element MeasurandType/EngineeringUnits

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
MN3
source | <xs:element name="EngineeringUnits" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>MN3</xs:documentation> </xs:annotation> </xs:element>

element MeasurandType/LinkType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | TmatsCommon:LinkTypeType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | PCM
facets |
enumeration | Analog
enumeration | PCM
enumeration | Other
annotation |
documentation
MN4
source | <xs:element name="LinkType" type="TmatsCommon:LinkTypeType" default="PCM" minOccurs="0"> <xs:annotation> <xs:documentation>MN4</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy