complexType AsynchronousDataMergeFormatType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
children | Name MaskAndPattern Supercom LocationDefinition Location Interval Length MSBLocation Parity Subcommutation
used by |
element | PCMFormatAttributesType/AsynchronousDataMergeFormat
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="AsynchronousDataMergeFormatType"> <xs:sequence minOccurs="0"> <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>ADM\DMN</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MaskAndPattern" type="MaskAndPatternType" minOccurs="0"> <xs:annotation> <xs:documentation>From ADM\MP. If this element is absent (implying a TMATS value of "N"), Chapter 4 recommendations are used. Otherwise, patterns are defined here.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Supercom" type="TmatsCommon:NonNegativeIntegerOrNo" minOccurs="0"> <xs:annotation> <xs:documentation>ADM1</xs:documentation> </xs:annotation> </xs:element> <xs:element name="LocationDefinition" type="TmatsCommon:PCMLocationDefinitionType" minOccurs="0"> <xs:annotation> <xs:documentation>ADM2</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Location" type="xs:string" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>ADM3</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Interval" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADM4</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Length" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADM5</xs:documentation> </xs:annotation> </xs:element> <xs:element name="MSBLocation" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADM6</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Parity" type="TmatsCommon:OddEvenNoneType" default="None" minOccurs="0"> <xs:annotation> <xs:documentation>ADM7</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Subcommutation" type="SubcommutationType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>ADM8. If absent, no subcommutation is present. Subcommutation fields include: ADM9, ADM10, ADM11</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element AsynchronousDataMergeFormatType/Name

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ADM\DMN
source | <xs:element name="Name" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>ADM\DMN</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/MaskAndPattern

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | MaskAndPatternType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | OverheadMask FreshDataPattern DataOverflowPattern StaleDataPattern UserDefinedPattern
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
From ADM\MP. If this element is absent (implying a TMATS value of "N"), Chapter 4 recommendations are used. Otherwise, patterns are defined here.
source | <xs:element name="MaskAndPattern" type="MaskAndPatternType" minOccurs="0"> <xs:annotation> <xs:documentation>From ADM\MP. If this element is absent (implying a TMATS value of "N"), Chapter 4 recommendations are used. Otherwise, patterns are defined here.</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/Supercom

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | TmatsCommon:NonNegativeIntegerOrNo
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ADM1
source | <xs:element name="Supercom" type="TmatsCommon:NonNegativeIntegerOrNo" minOccurs="0"> <xs:annotation> <xs:documentation>ADM1</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/LocationDefinition

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | TmatsCommon:PCMLocationDefinitionType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | First Word And Interval
enumeration | Every Location
enumeration | Contiguous Words
enumeration | Not Applicable
annotation |
documentation
ADM2
source | <xs:element name="LocationDefinition" type="TmatsCommon:PCMLocationDefinitionType" minOccurs="0"> <xs:annotation> <xs:documentation>ADM2</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/Location

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 1
maxOcc | unbounded
content | simple
annotation |
documentation
ADM3
source | <xs:element name="Location" type="xs:string" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>ADM3</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/Interval

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ADM4
source | <xs:element name="Interval" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADM4</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/Length

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ADM5
source | <xs:element name="Length" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADM5</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/MSBLocation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | xs:positiveInteger
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
ADM6
source | <xs:element name="MSBLocation" type="xs:positiveInteger" minOccurs="0"> <xs:annotation> <xs:documentation>ADM6</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/Parity

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | TmatsCommon:OddEvenNoneType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
default | None
annotation |
documentation
ADM7
source | <xs:element name="Parity" type="TmatsCommon:OddEvenNoneType" default="None" minOccurs="0"> <xs:annotation> <xs:documentation>ADM7</xs:documentation> </xs:annotation> </xs:element>

element AsynchronousDataMergeFormatType/Subcommutation

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsPGroup.xsd
type | SubcommutationType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | StartFrame FrameInterval EndFrame
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
ADM8. If absent, no subcommutation is present. Subcommutation fields include: ADM9, ADM10, ADM11
source | <xs:element name="Subcommutation" type="SubcommutationType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>ADM8. If absent, no subcommutation is present. Subcommutation fields include: ADM9, ADM10, ADM11</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy