complexType TelemetryValueDefinitionType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
children | BinaryFormat FloatingPointFormat BitWeight
used by |
element | MeasurementType/TelemetryValueDefinition
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:complexType name="TelemetryValueDefinitionType"> <xs:sequence minOccurs="0"> <xs:element name="BinaryFormat" type="TmatsCommon:BinaryFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>BFM</xs:documentation> </xs:annotation> </xs:element> <xs:choice minOccurs="0"> <xs:annotation> <xs:documentation>Choice, depending on BFM value</xs:documentation> </xs:annotation> <xs:element name="FloatingPointFormat" type="TmatsCommon:FloatingPointFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>FPF</xs:documentation> </xs:annotation> </xs:element> <xs:element name="BitWeight" type="BitWeightType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Used when BFM value = "BWT". Repeats "BWT\N" times</xs:documentation> </xs:annotation> </xs:element> </xs:choice> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion"/> </xs:complexType>

element TelemetryValueDefinitionType/BinaryFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | TmatsCommon:BinaryFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | Integer
enumeration | Unsigned Binary
enumeration | Sign and Magnitude Binary (+=0)
enumeration | Sign and Magnitude Binary (+=1)
enumeration | One's Complement
enumeration | Two's Complement
enumeration | Offset Binary
enumeration | Floating Point
enumeration | Binary Coded Decimal
enumeration | Bit Weight
enumeration | Other
annotation |
documentation
BFM
source | <xs:element name="BinaryFormat" type="TmatsCommon:BinaryFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>BFM</xs:documentation> </xs:annotation> </xs:element>

element TelemetryValueDefinitionType/FloatingPointFormat

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | TmatsCommon:FloatingPointFormatType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
facets |
enumeration | IEEE 754 Single Precision
enumeration | IEEE 754 Double Precision
enumeration | MIL STD 1750A Single Precision
enumeration | MIL STD 1750A Double Precision
enumeration | DEC Single Precision
enumeration | DEC Double Precision
enumeration | DEC G Double Precision
enumeration | IBM Single Precision
enumeration | IBM Double Precision
enumeration | TI Single Precision
enumeration | TI Extended Precision
annotation |
documentation
FPF
source | <xs:element name="FloatingPointFormat" type="TmatsCommon:FloatingPointFormatType" minOccurs="0"> <xs:annotation> <xs:documentation>FPF</xs:documentation> </xs:annotation> </xs:element>

element TelemetryValueDefinitionType/BitWeight

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsCGroup.xsd
type | BitWeightType
properties |
isRef | 0
minOcc | 0
maxOcc | unbounded
content | complex
children | BitNumber BitWeightValue
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
Used when BFM value = "BWT". Repeats "BWT\N" times
source | <xs:element name="BitWeight" type="BitWeightType" minOccurs="0" maxOccurs="unbounded"> <xs:annotation> <xs:documentation>Used when BFM value = "BWT". Repeats "BWT\N" times</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy