complexType MultiplexModulationGroupType

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
children | TmatsM:CompositeSignalStructure TmatsM:BasebandSignal TmatsM:Subcarriers TmatsM:ReferenceChannel TmatsM:DataConversionAttributes TmatsM:Comments
used by |
element | DataSourceType/MultiplexModulationGroup
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
TMATS M-Group
source | <xs:complexType name="MultiplexModulationGroupType"> <xs:annotation> <xs:documentation>TMATS M-Group</xs:documentation> </xs:annotation> <xs:sequence minOccurs="0"> <xs:element name="CompositeSignalStructure" type="TmatsM:CompositeSignalStructureType" minOccurs="0"/> <xs:element name="BasebandSignal" type="TmatsM:BasebandSignalType" minOccurs="0"/> <xs:element name="Subcarriers" type="TmatsM:SubcarriersType" minOccurs="0"/> <xs:element name="ReferenceChannel" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>RC</xs:documentation> </xs:annotation> </xs:element> <xs:element name="DataConversionAttributes" type="TmatsC:DataConversionAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>for FM links only</xs:documentation> </xs:annotation> </xs:element> <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> <xs:attribute ref="TmatsCommon:TmatsVersion" use="required"/> </xs:complexType>

element MultiplexModulationGroupType/CompositeSignalStructure

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | CompositeSignalStructureType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsM:SignalStructureType TmatsM:ModulationSense TmatsM:CompositeLPFBandwidth
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="CompositeSignalStructure" type="TmatsM:CompositeSignalStructureType" minOccurs="0"/>

element MultiplexModulationGroupType/BasebandSignal

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | BasebandSignalType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsM:SignalType TmatsM:LowPassFilter TmatsM:DataLinkName TmatsM:MeasurementName
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="BasebandSignal" type="TmatsM:BasebandSignalType" minOccurs="0"/>

element MultiplexModulationGroupType/Subcarriers

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | SubcarriersType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | TmatsM:IRIGSubcarrier TmatsM:Other
attributes |
Name | Type | Use | Default | Fixed | annotation
TmatsVersion |  |  |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
source | <xs:element name="Subcarriers" type="TmatsM:SubcarriersType" minOccurs="0"/>

element MultiplexModulationGroupType/ReferenceChannel

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
RC
source | <xs:element name="ReferenceChannel" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>RC</xs:documentation> </xs:annotation> </xs:element>

element MultiplexModulationGroupType/DataConversionAttributes

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | DataConversionAttributesType
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | complex
children | Measurement
attributes |
Name | Type | Use | Default | Fixed | annotation
ID |  | required |  |  |
documentation
Added in 106-15 at the request of MDL for C,D,P,B groups
TmatsVersion |  | required |  |  |
documentation
The IRIG version this document conforms to
documentation
Added 106-15 as an option
annotation |
documentation
for FM links only
source | <xs:element name="DataConversionAttributes" type="TmatsC:DataConversionAttributesType" minOccurs="0"> <xs:annotation> <xs:documentation>for FM links only</xs:documentation> </xs:annotation> </xs:element>

element MultiplexModulationGroupType/Comments

diagram |
namespace | http://www.wsmr.army.mil/RCCsite/Documents/106-15_Telemetry_Standards/schemas/TMATS/TmatsMGroup.xsd
type | xs:string
properties |
isRef | 0
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
COM
source | <xs:element name="Comments" type="xs:string" minOccurs="0"> <xs:annotation> <xs:documentation>COM</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy